{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["標價清單 明細表 ","標價清單 單價分析"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":14,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"標價清單 明細表 ","index":0,"n_rows":481,"n_cols":7,"rows_kept":481,"cut":false,"hidden":false,"merged":[[23,1,23,5],[33,1,33,6],[28,1,28,6],[29,1,29,6],[30,1,30,6],[31,1,31,6],[32,1,32,6],[343,1,343,3],[24,1,24,6],[25,1,25,6],[26,1,26,6],[27,1,27,6]]}
["項次","名                稱","單位","數   量","單   價","複    價","備    註"]
["壹","建築土木工程"]
["一","假設工程","式",1]
["二","地下開挖安全措施","式",1]
["三","RC結構工程","式",1]
["四","鋼構工程","式",1]
["五","外牆裝修工程","式",1]
["六","室內一般裝修工程","式",1]
["七","門窗工程(含玻璃及門窗五金)","式",1]
["八","雜項工程","式",1]
["九","電梯設備工程(含吊掛鋼樑等安裝須求項目)","式",1]
["十","景觀及植栽工程","式",1]
["十一","其他工程(漏列項目)","式",1]
[null,"小計(一~十一)"]
["十二","勞工安全衛生管理費","式",1]
["十三","交通維持、道路維護費及環境保護費","式",1]
["十四","施工品質管制作業費及材料檢驗測試費","式",1]
["十五","承包商利潤、管理及保險費","式",1]
[null,"小計 (十一~十五)"]
[null,"合計 (一~十五)"]
["十六","加值營業稅 5%","式",1]
[null,"總計 (一~十六)"]
[]
[null,"工程總價:新台幣   億   仟   佰   拾   萬   仟   佰   拾   元整(含稅)"]
[null,"註:  1. 所有材料廠牌型號品質標準依據，廠商可依相同品質認証材料送審,未經業主同意不得使用於"]
[null,"        本建築內，標單所列項目、數量僅供參考，廠商投標前應自行按圖詳估，如發現與圖說有出入"]
[null,"        等情形，應合併於單價內或其他相關項目內估計之。"]
[null,"     2. 投標時需提報施工計劃。"]
[null,"     3. 使照申請時配合施作工項\"廠商應依相關圖說自行增列項目並詳估費用。"]
[null,"     4. 廠商須依圖說及標單項目內容評估屬一次性工項或配合使照申請分階段完成之工項自行估算"]
[null,"        該工項之合理單價填入。"]
[null,"     5.工地使用之鋼管施工架應全面符合國家標準CNS 4750及相關勞安衛規定。"]
[null,"     6.本工程檢、試驗含於總價內，其試驗項目及次數，以施工圖說及公共工程施工規範為主。"]
[null,"     7.營造公司負責本案使用執照之申辦及取得，並完成正式用水用電，為本工程之一部分。"]
["壹","土木建築工程"]
["一","假設工程"]
[1,"基地清理及整地(高程整至GL0)","M2",4457]
[2,"全阻隔式安全圍籬，H=2.4M,30cm止水墩,警示燈及警示標誌－施工期間維護","M",248,null,null,"部分已施作"]
[3,"施工圍籬綠美化－施工期間保活養護","M",49,null,null,"部分已施作"]
[4,"施工圍籬，折疊式大門，8M，(含地坪混凝土鋪設)－施工期間維護","樘",1,null,null,"部分已施作"]
[5,"環境保護，沖洗設備，(臨時洗車台設備及防污設備)－施工期間維護","處",1,null,null,"部分已施作"]
[6,"廠區駐地警衛保全及崗亭","處",1]
[7,"工地臨時辦公室(含水電設備及傢俱)","式",1]
[8,"工地臨時移動廁所，含日常清潔","座",4]
[9,"工地臨時給排水,電，照明，監視設備及臨時水電費","式",1]
[10,"施工中安全防護﹑警示措施及設備費(含各種開口),消防設施","式",1]
[11,"環境保護，灑水設施，各項汙染物防制及設置費(含營建工地逕流廢水污染削減計畫書)","式",1]
[12,"營建廢棄物及垃圾運棄及吊運費","式",1]
[13,"施工之臨時抽排水費","式",1]
[14,"工程告示牌(W=60cm,L=85cm)－施工期間維護","面",1,null,null,"部分已施作"]
[15,"工程攝錄影，紀錄片後製及報表相片等費用","式",1]
[16,"完工交屋前清潔費","式",1]
[17,"鄰房鑑定費","式",1]
[18,"工程介面整合圖說及施工圖繪製","式",1]
[19,"樓層勘驗，使照請領費用","式",1]
[20,"全區臨時照明含地下室施工照明設備","式",1]
[21,"公共設施復原(施工及申請)","式",1]
[22,"外部施工鷹架含安全網 含斜籬","M2",15103]
[23,"室內高層及挑空區週邊工作架 >4.5M","M2",8420]
[24,"高空工作車及移動工作架(建築裝修)","式",1]
[null,"  計"]
["備註:","施工電梯由營造自行評估，不另計價，費用自行加入"]
[null,"施工塔吊由營造自行評估，不另計價，費用加入鋼構吊裝內"]
[]
["二","地下開挖安全措施"]
["1","擋土型鋼 H300*300*10*15 @50 L=14M","支",225]
["2","擋土型鋼 H300*300*10*15 @50 L=16M","支",205]
["3","H300 中間樁 L=13(含止水板及截樁3.6M)","支",36]
["4","H300 中間樁 L=15(含止水板及截樁3.75M)","支",36]
["5","第一層H型鋼橫擋及支撐 H-350*350*12*19 含H350圍令","M2",2903]
["6","第二層H型鋼橫擋及支撐 H-400*400*13*21 含H400圍令","M2",2903]
["7","第三層H型鋼橫擋回撐 H-400*400*13*21 含H400圍令","M2",1133]
["8","施工輔助，施工構台","M2",495]
["9","構台及四週安全欄杆,安全母索,施工便梯","M",435]
["10","挖方(含警衛室)","M3",28661]
["11","廢方運棄及土方處理費(含警衛室)","M3",26081]
["12","現地土方回填(含警衛室)","M3",2580]
["13","安全監測系統","式",1]
[null,"  計"]
[]
["三","RC結構工程"]
[1,"施工測量，放樣","M2",20177]
[2,"結構用混凝土 140kgf/cm2","M3",264]
[3,"結構用混凝土 280kgf/cm2","M3",6736]
[4,"結構用混凝土 350kgf/cm2","M3",2974]
[5,"筏基內回填低強度混凝土 105kgf/cm2","M3",1161]
[6,"鋼筋，SD420W","噸",1346]
[7,"鋼絲網10*8/100*100&10*10/100*100","T",187]
[8,"普通模板","M2",25953]
[9,"平頂清水模板","M2",5960]
[10,"閉口型鋼承板 高65*1.2","M2",16146]
[11,"#6接鋼柱  鋼筋續接器","組",12]
[12,"#8 鋼筋續接器","組",344]
[13,"#10 鋼筋續接器","組",1082]
[14,"#10接鋼柱  鋼筋續接器","組",90]
[15,"#6 T頭 ","組",348]
[16,"#8 T頭 ","組",200]
[17,"#10 T頭 ","組",944]
[18,"接鋼柱剪力釘 19∮*200","支",3431]
[19,"複合型橡膠鋼板止水帶","M",409]
[null,"  計"]
[]
["四","鋼構工程"]
[1,"鋼板焊接口型鋼 SN490B","T",1111.2]
[2,"BH及RH型鋼 SN490B","T",1049.7]
[3,"H型鋼 A572","T",434.4]
[4,"H型鋼 A36","T",34.299999999999997]
[5,"鋼板 SN490B,A572","T",248.5]
[6,"鋼板 A36","T",13.5]
[7,"角鋼","T",2.6]
[8,"預埋螺栓 L=700 M-36A.B","支",116]
[9,"預埋螺栓 L=600 M24 A.B","支",96]
[10,"S10T 扭矩控制螺栓","T",31.2]
[11,"25∮TIE 拉桿","支",4060]
[12,"剪力釘 19∮*76","支",16856]
[13,"剪力釘 19∮*100","組",94581]
[14,"柱內灌漿混凝土(含工料)","M3",416]
[15,"不收縮砂漿","M3",0.9]
[16,"結構鋼構吊裝(含吊裝機具設備及現場焊接及設備)","T",2894]
[17,"鋼料半成品運費及工地小搬運","T",2894]
[18,"鋼樑工廠開孔補強","孔",226]
[19,"鋼樑小樑工廠開孔補強","孔",356]
[20,"鋼樑一小時防火漆","M2",7909]
[21,"鋼樑二小時防火漆","M2",11007]
[22,"鋼柱一小時防火漆(含屋面以上構架)","M2",2106]
[23,"鋼柱二小時防火漆","M2",2404]
[24,"H型鋼柱一小時防火漆","M2",639]
[25,"H型鋼柱二小時防火漆","M2",885]
[26,"室內鋼樓梯 ","T",82]
[27,"樓梯 鋼筋網","M2",705]
[28,"樓梯 面層混凝土 280kg/cm2","M3",30]
[29,"電梯昇降道內中間鋼樑","T",8]
[null,"  計"]
[]
["五","外牆裝修工程"]
[1,"外牆造型2.5mm氟碳烤漆鋁包板牆(含雨遮及各種飾板)","M2",6455]
[2,"外牆4mm氟碳烤漆鋁複合板包板牆","M2",5562]
[3,"防火層間塞","M",1110]
[4,"外牆貼45mm*45mm小口磚","M2",310]
[5,"警衛室窗台板貼花崗石","M2",5.4]
[6,"氟碳烤漆金屬格柵裝飾牆","M2",477]
[7,"氣體區氟碳烤漆金屬格柵牆","M2",19]
[8,"氣體區氟碳烤漆不銹鋼單片橫拉門 125*226","樘",1]
[9,"二層建築物出入口雨遮之不銹鋼排水溝(厚度2.0mm)，兩側80mm∮高籠型落水頭及100mm∮RP，排水至鄰近雨水幹管。","式",1]
[null,"  計"]
[]
["六","室內一般裝修工程"]
[1,"高層纖維水泥板灌漿隔間","M2",447]
[2,"一般樓層纖維水泥板灌漿隔間","M2",1252]
[3,"纖維水泥板廁所外側單面封板","M2",587]
[4,"高層雙面矽酸鈣板防火隔間牆","M2",1091]
[5,"一般樓層雙面矽酸鈣板防火隔間牆","M2",3489]
[6,"鋁帷幕牆內側單面封牆","M3",1233]
[7,"外牆內側金屬庫板隔間牆","M2",627]
[8,"一小時防火時效金屬庫板牆(挑空區管道間)","M2",453]
[9,"牆面1:3水泥粉刷","M2",1070]
[10,"輕隔間牆面批土整平","M2",1845]
[11,"牆面1:3水泥粉刷批土刷水泥漆","M2",6714]
[12,"地下室外側牆面1:2防水泥粉刷刷水泥漆","M2",1066]
[13,"輕隔間牆面批土刷水泥漆","M2",7003]
[14,"輕隔間牆面補強乾式吊掛石材","M2",31]
[15,"RC牆面乾掛石材","M2",152]
[16,"廁所牆面1:2水泥砂漿貼30*60磁磚","M2",267]
[17,"廁所輕隔間牆面黏著劑貼30*60磁磚","M2",1075]
[18,"廁所牆面150CM高防水塗佈","M2",647]
[19,"牆面無毒防水劑+防水粉刷貼20*20面磚","M2",36]
[20,"踢腳水泥粉刷水泥漆,10CM","M",2774]
[21,"踢腳刷環氧樹脂 10CM","M",420]
[22,"踢腳刷環氧樹脂 20CM","M",878]
[23,"地坪乾式打底貼拋光面石材","M2",843]
[24,"地坪1:3水泥砂漿貼60*60抛光石英磚","M2",669]
[25,"地坪高平整拍漿粉光耐磨型環氧樹脂地坪,厚度3mm","M2",3324]
[26,"斜車道整體粉光止滑型環氧樹脂,厚度5mm","M2",691]
[27,"地坪高平整拍漿粉光平滑型環氧樹脂地坪,厚度3mm","M2",10650]
[28,"樓梯面貼20*20面磚+止滑磚","M2",178]
[29,"樓梯面貼PVC地磚+止滑條","M2",891]
[30,"廁所地坪防水塗佈後貼30*30止滑石英磚","M2",369]
[31,"無毒防水劑+1:2防水粉刷貼20*20地磚","M2",32]
[32,"地坪高平整整體粉光","M2",148]
[33,"樓梯地坪收邊抿石子","M2",12]
[34,"地坪高平整整體粉光加自平泥面貼60*60cmPVC透心地磚","M2",1712]
[35,"平頂未施作材料表面清潔(含溢漿清理)","M2",13839]
[36,"平頂清水模面噴水泥漆","M2",3577]
[37,"平頂樑底樑側清水模面噴水泥漆","M2",1991]
[38,"平頂水泥粉刷水泥漆(含樑底樑側)","M2",198]
[39,"鋼樓梯背板噴漆(含側板)","M2",1041]
[40,"樓電梯位置磚","M2",12]
[41,"筏基內水池地坪牆面防水塗佈後加七厘石防水粉刷","M2",1939]
[42,"筏基空調及製程水池地坪牆面防水粉刷貼20*20面磚","M2",713]
[43,"屋面及露台防水隔熱層","M2",1972]
[44,"屋面1/2B汎水壓磚","M",390]
[45,"女兒牆內側防水粉刷(含汎水)","M2",428]
[46,"屋頂平台排水溝鋪設高腳隔熱磚(長度30cm*寬度30cm*高度5.5cm)","M",183]
[47,"地下室頂板防水層含保護層","M2",704]
[48,"筏基及一層外推地坪防潮層","M2",2941]
[49,"地下室外牆接縫防水打鑿","M",818]
[50,"地下室外牆防水層","M2",2022]
[51,"屋面設備基座 15CM高","M2",78]
[52,"屋面鋁制排水盤","個",42]
[53,"屋頂女兒牆笠木蓋板收邊","M",110]
[54,"屋頂平台排水溝鋪設高密度聚乙烯導水板(厚度10MM，上層附PET熱熔不織布)+卵石(直徑2~3cm)","M2",4]
[55,"RC外牆處窗框四周(30CM)防水層","M2",9]
[56,"屋頂及露台女兒牆泛水收邊下立牆牆面防水設施","M2",170]
[null,"  計"]
[]
["七","門窗工程(含玻璃及門窗五金)"]
[1,"D1 200*235 不銹鋼烤漆安全門 F60A (遮煙)","樘",1]
[2,"D2 120*220 不銹鋼烤漆安全門 F60A (遮煙)","樘",36]
[3,"D3 120*220 不銹鋼烤漆安全門 F60A (遮煙)","樘",1]
[4,"D4 250*250 不銹鋼烤漆防火門 F60A (遮煙)","樘",1]
[5,"D5 240*220 不銹鋼烤漆防火門 F60A (遮煙)","樘",14]
[6,"D6 240*220 不銹鋼烤漆防火門 F60A (遮煙)","樘",2]
[7,"D7 200*235 不銹鋼烤漆安全門 F60A (遮煙)","樘",1]
[8,"D8 200*220 不銹鋼烤漆防火門 F60A (遮煙)","樘",11]
[9,"D9 120*220 不銹鋼烤漆防火門 F60A (遮煙)","樘",3]
[10,"D10 100*220 不銹鋼烤漆防火門 F60A (遮煙)","樘",12]
[11,"D11 160*210 不銹鋼烤漆防火門 F60A (遮煙)","樘",45]
[12,"D12 160*200 不銹鋼烤漆防火門 F60A (遮煙)","樘",2]
[13,"D13 90*210 不銹鋼烤漆防火門 F60A (遮煙)","樘",18]
[14,"D14 300*300 不銹鋼烤漆防火門 F60A","樘",1]
[15,"D15 250*250 不銹鋼烤漆防火門 F60A","樘",2]
[16,"D16 240*220 不銹鋼烤漆防火門 F60A","樘",1]
[17,"D17 200*220 不銹鋼烤漆防火門 F60A","樘",4]
[18,"D18 120*220 不銹鋼烤漆防火門 F60A","樘",6]
[19,"D19 100*220 不銹鋼烤漆防火門 F60A","樘",2]
[20,"D20 200*220 不銹鋼烤漆門 ","樘",1]
[21,"D21 120*220 不銹鋼烤漆門","樘",1]
[22,"D22 120*220 不銹鋼烤漆門","樘",2]
[23,"D23 100*220 鋼製烤漆門 含視窗","樘",1]
[24,"D24 90*220 鋼製烤漆門 含視窗","樘",27]
[25,"D25 80*210 鋼製烤漆門 含百葉","樘",1]
[26,"D26 200*205 不銹鋼烤漆門 台電規格橫拉門 ","樘",1]
[27,"D27 110*210 SMC 無障礙拉門","樘",4]
[28,"D28 120*120 不銹鋼防火維修門 F60B","樘",13]
[29,"D29 80*120 不銹鋼防火維修門 F60B","樘",13]
[30,"SD1  700*322  不銹鋼電動捲門","樘",1]
[31,"SD2  310*445  不銹鋼電動捲門","樘",2]
[32,"SD3  350*400  不銹鋼電動捲門","樘",1]
[33,"SD4  350*375  不銹鋼電動捲門","樘",8]
[34,"SD5  500*280  不銹鋼電動防火捲門 60A","樘",1]
[35,"SD6  181*280  遮煙捲簾","樘",18]
[36,"L1 鍍鋅鋼板防火百葉閘門 65*65","樘",1]
[37,"L1a 鍍鋅鋼板防火百葉閘門 65*65","樘",1]
[38,"L2 284*156 防颱型鋁百葉","樘",1]
[39,"L3 134*156 防颱型鋁百葉","樘",4]
[40,"L4 140*200 防颱型鋁百葉","樘",1]
[41,"L5 250*100 防颱型鋁百葉","樘",1]
[42,"L6 1100*100 防颱型鋁百葉+鋁窗","樘",3]
[43,"L7 85*150 防颱型鋁百葉","樘",2]
[44,"L8 100*100 可關閉防水型鋁百葉","樘",1]
[45,"L8a 100*100 可關閉防水型鋁百葉","樘",2]
[46,"L9 60*60 防颱型鋁百葉","樘",1]
[47,"L9a 60*60 防颱型鋁百葉","樘",1]
[48,"L10 130*55 防颱型鋁百葉","樘",1]
[49,"W1 1100*200 鋁窗 (附摺疊紗窗)","樘",1]
[50,"W2 1100*100 鋁窗 (附摺疊紗窗)","樘",5]
[51,"W3 300*200 鋁窗 (附摺疊紗窗)","樘",1]
[52,"W4 180*100 鋁窗 (附摺疊紗窗)","樘",1]
[53,"W4a 180*100 鋁窗 (附摺疊紗窗)","樘",1]
[54,"W5 180*100 鋁窗+防颱型百葉 (附摺疊紗窗)","樘",1]
[55,"W6 100*100 鋁窗 (附摺疊紗窗)","樘",2]
[56,"W6a 100*100 鋁窗 (附摺疊紗窗)","樘",18]
[57,"W7 100*50 鋁窗 (附摺疊紗窗)","樘",4]
[58,"W8 840*245 鋁窗+鋁門 (附紗窗,紗門)","樘",1]
[59,"W9 100*100 鋁窗 (附紗窗)","樘",1]
[60,"CW1 1214*4845 玻璃帷幕牆 含飾板","樘",1]
[61,"CW2 3980.5*1185 玻璃帷幕牆","樘",1]
[62,"CW3 219.5*490 玻璃帷幕牆","樘",1]
[63,"CW4 219.5*490 玻璃帷幕牆 ","樘",1]
[64,"CW5 1498*400 玻璃帷幕牆 風除室","樘",1]
[65,"CW6 979*335 玻璃帷幕牆","樘",1]
[66,"CW7 994*345 玻璃帷幕牆","樘",2]
[67,"CW8 898*345 玻璃帷幕牆","樘",1]
[68,"CW9 979*200 玻璃帷幕牆","樘",6]
[69,"CW10 968*305 玻璃帷幕牆","樘",1]
[70,"CW11 980*305 玻璃帷幕牆","樘",1]
[71,"CW12 1691*360 玻璃帷幕牆","樘",1]
[72,"CW13 180*5010 玻璃帷幕牆","樘",1]
[73,"CW14 242*4110 玻璃帷幕牆","樘",1]
[74,"CW15 3424*434*6 玻璃帷幕牆 含鋁飾板","樘",1]
[null,"  計"]
[]
["八","雜項工程"]
[1,"無障礙安全梯A無障礙樓梯扶手TYPE A(H=90cm)","M",361]
[2,"無障礙安全梯A無障礙樓梯扶手TYPE B(H=110cm)","M",2]
[3,"無障礙安全梯A無障礙壁掛式扶手 安裝H=75cm","M",8]
[4,"安全梯B樓梯扶手TYPE A(H=90cm)","M",238]
[5,"安全梯B樓梯扶手TYPE B(H=110cm)","M",2]
[6,"安全梯C樓梯扶手TYPE A(H=90cm)","M",92]
[7,"安全梯C樓梯扶手TYPE B(H=110cm)","M",1]
[8,"B2,B1層階梯無障礙樓梯扶手TYPE A(H=90cm)","M",8]
[9,"B2,B1階梯無障礙壁掛式扶手 安裝H=75cm","M",8]
[10,"上電梯機房階梯樓梯扶手TYPE A(H=90cm)","M",3]
[11,"吊裝平台不銹鋼活動欄杆","M",69]
[12,"組合式防水閘門(長度790cm*高度90cm)","組",1]
[13,"筏基水池氣密鑄鐵人孔蓋 80∮","組",21]
[14,"筏基水箱不銹鋼爬梯 H*1.5","組",21]
[15,"電梯坑不銹鋼爬梯","組",5]
[16,"屋面不銹鋼人孔蓋 80*80","座",2]
[17,"屋面不銹鋼爬梯 H=404CM","座",1]
[18,"屋面不銹鋼爬梯 H=354CM","座",1]
[19,"廁所熱固性板隔間 含門扇,五金,掛鈎","間",61]
[20,"小便斗隔板","片",21]
[21,"單元廁所馬桶背板及上方蓋板(含鍍鋅鐵件)","組",41]
[22,"單元小便斗背板(含鍍鋅鐵件)","組",31]
[23,"小便斗上方人造石蓋板","M",29]
[24,"無障礙小便斗扶手","組",11]
[25,"無障礙廁所扶手配件","間",4]
[26,"人造石洗手台面","M",34]
[27,"三重明鏡","M2",27]
[28,"茶水間組合式系統櫃含水槽及吊櫃 L=225CM","座",10]
[29,"汽車停車位劃線","個",84]
[30,"無障礙汽車停車位劃線(含標誌,共用走道)","個",2]
[31,"機車停車位劃線","個",79]
[32,"無障礙機車位劃線(含標誌)","個",2]
[33,"一樓裝卸車位劃線","個",2]
[34,"車輪檔","個",172]
[35,"防撞條","個",141]
[36,"反射鏡","個",5]
[37,"方向箭頭","個",6]
[38,"車道截水溝","M",8]
[39,"筏基連通管 6\"","支",82]
[40,"筏基通氣管 4\"","支",82]
[41,"壁面LOGO廣告招牌(含吊車安裝)","式",1]
[42,"建築銘牌","式",1]
[43,"公共藝術品說明牌 80*50cm","式",1]
[44,"地面招牌含基座","式",1]
[45,"休閒座椅","座",2]
[46,"內徑∮30cm高壓水泥涵管","M",222]
[47,"陰井","座",43]
[48,"高壓混凝土路緣石(噴砂面)60*15*20cm","M",29]
[49,"地下水箱不銹鋼人孔蓋 80*80","座",1]
[50,"地下水箱外側不銹鋼爬梯 H=220CM","座",1]
[51,"地下水箱內側不銹鋼爬梯 H=150CM","座",1]
[52,"無障礙停車位立牌型(含基座)","座",4]
[53,"無障礙停車位引導立牌型(含基座)","組",1]
[54,"無障礙引導標誌-懸掛式長版","組",10]
[55,"無障礙引導標誌-懸掛式短版","組",26]
[56,"無障礙引導標誌-張貼式","組",25]
[57,"吊牆(具一小防火時效，高度80cm，含防火填塞)","M2",281]
[58,"管道間熱浸鍍鋅格柵板工作道(含扶手及固定鍍鋅鐵件等，寬度(含扶手)60cm)","M2",92]
[59,"電動柵欄機，檔桿長度5m，含RC基座。","座",2]
[null,"  計"]
[null,"廁所設備,馬桶,小便斗等型式由業主決定,並由機電廠商施作"]
[null,"充電樁規格採DC快充型式,由機電廠商建置"]
[]
["九","電梯設備工程(含吊掛鋼樑等安裝須求項目)"]
[1,"乘客兼無障礙電梯 1000KG 90M/Min 12停","部",1]
[2,"乘客梯 1000KG 90M/Min 12停","部",1]
[3,"載貨電梯 3000KG 60M/Min 13停","部",1]
[4,"乘客載貨電梯 雙向門 1000KG 90M/Min 9停","部",2]
[5,"卸貨平台月台調整板(電動油壓式)W1600*L2000*H500mm","部",2]
[null,"  計"]
[]
["十","景觀及植栽工程"]
[1,"景觀假設工程"]
["1.1","放樣","M2",2455]
["1.2","整地","M2",2455]
["1.3","警示措施","式",1]
["1.4","喬木苦楝現地移植入空氣盆，後定植 (H>300cm,W=250cm,∮>5cm)","株",1]
["1.5","現況雜草石塊垃圾移除運棄","式",1]
[null,"  計"]
[2,"植栽工程 "]
["2.1","喬木-樟樹((H>600cm,W=400cm,∮>15cm) 苗木費","株",1]
["2.2","喬木-樟樹((H>500cm,W=300cm,∮>12cm) 苗木費","株",2]
["2.3","喬木-竹柏 ((H>400cm,W=200cm,∮>6cm) 苗木費","株",17]
["2.4","喬木-青剛櫟((H>400cm,W=250cm,∮>10cm) 苗木費","株",1]
["2.5","喬木-台灣山櫻((H>400cm,W=400cm,∮>15cm) 苗木費","株",12]
["2.6","喬木-青楓((H>400cm,W=350cm,∮>15cm) 苗木費","株",1]
["2.7","喬木-黃連木((H>350cm,W=250cm,∮>10cm) 苗木費","株",1]
["2.8","喬木-整形羅漢松((H>350cm,W=250cm,∮>10cm) 苗木費","株",1]
["2.9","喬木-半自然形羅漢松((H>300cm,W=250cm,∮>6cm) 苗木費","株",2]
["2.10","喬木-錐形羅漢松((H>300cm,W=250cm,∮>6cm) 苗木費","株",28]
["2.11","喬木種植費","株",66]
["2.12","灌木-黃金五爪木(H=50cm,W=50cm) 苗木費","株",36]
["2.13","灌木-黃金串錢柳(H=30cm,W=20cm) 苗木費","株",178]
["2.14","灌木-樹蘭(H=25cm,W=20cm) 苗木費","株",163]
["2.15","灌木-吊蘭(H=20cm,W=20cm) 苗木費","株",790]
["2.16","灌木-巴西鳶尾(H=40cm,W=30cm) 苗木費","株",263]
["2.17","灌木-熊貓仙丹(H=20cm,W=20cm) 苗木費","株",118]
["2.18","灌木-矮旭仙丹(H=20cm,W=20cm) 苗木費","株",130]
["2.19","灌木-斑葉桔梗蘭(H=30cm,W=20cm) 苗木費","株",128]
["2.20","灌木-細葉杜鵑(H=15cm,W=15cm) 苗木費","株",8672]
["2.21","灌木-平戶杜鵑(H=40cm,W=30cm) 苗木費","株",699]
["2.22","灌木-偃柏(H=30cm,W=60cm) 苗木費","株",154]
["2.23","灌木-斑葉海桐(H=30cm,W=30cm) 苗木費","株",232]
["2.24","灌木-台灣野牡丹藤(H=40cm,W=30cm) 苗木費","株",529]
["2.25","灌木-矮性翠盧莉(H=15cm,W=15cm) 苗木費","株",1111]
["2.26","灌木-錫蘭葉下珠(H=15cm,W=15cm) 苗木費","株",240]
["2.27","灌木-百子蓮(H=40cm,W=30cm) 苗木費","株",183]
["2.28","灌木-翠米茶(H=20cm,W=20cm) 苗木費","株",110]
["2.29","灌木-斑葉鵝掌藤(H=40cm,W=30cm) 苗木費","株",144]
["2.30","灌木-細葉七里香(H=20cm,W=20cm) 苗木費","株",110]
["2.31","灌木-蜘蛛百合(H=40cm,W=30cm) 苗木費","株",125]
["2.32","灌木-早乙女杜鵑(H=10cm,W=10cm) 苗木費","株",721]
["2.33","灌木-白鶴芋(H=50cm,W=30cm) 苗木費","株",106]
["2.34","灌木-南天竹(H=120cm,W=50cm) 苗木費","株",5]
["2.35","灌木-細葉觀音棕竹(H=180cm,W=80cm) 苗木費","株",3]
["2.36","灌木-球型細葉七里香(H=50cm,W=40cm) 苗木費","株",2]
["2.37","灌木-球型細葉七里香(H=70cm,W=60cm) 苗木費","株",2]
["2.38","灌木-球型細葉七里香(H=90cm,W=80cm) 苗木費","株",2]
["2.39","灌木種植費","株",14956]
["2.40","地被-類地毯草(密鋪)","M2",485]
["2.41","地被-銀紋沿階草(H=30cm,W=20cm) 苗木費","株",211]
["2.42","地被-韭蘭(H=10cm,W=10cm) 苗木費","株",558]
["2.43","地被-玉龍草(H=6cm,W=6cm) 苗木費","株",2558]
["2.44","地被-種植費","株",3327]
["2.45","植栽，客土，砂質壤土 ","M3",460]
[null," 計"]
[]
[3,"鋪面工程 "]
["3.1","燒面花崗岩-60*60CM(黑灰)","M2",41]
["3.2","噴砂面高壓混凝土磚-30*30CM*8CM(白)","M2",791.2]
["3.3","噴砂面高壓混凝土磚-30*30CM*8CM(灰)錯落排列","M2",10.71]
["3.4","噴砂面高壓混凝土磚-30*30CM*8CM(灰)線性排列","M2",63.65]
["3.5","噴砂面高壓混凝土磚-30*30CM*8CM(黑灰)線性排列","M2",61.23]
["3.6","噴砂面高壓混凝土磚-10*10CM*8CM(黑灰)","M2",7.6]
["3.7","燒面花崗岩緣石-寬15CM(黑灰)T=8CM","M",209]
["3.8","玄武岩踏片步道","M2",21.8]
["3.9","入口處人行道鋪面復原(高壓混凝土磚40x20cm，TH=8cm丁掛排列，表面處理及顏色同現有人行道)","M2",24]
[null," 計"]
[4,"噴灌工程 "]
["4.1","RAINBIRD 1/2\"小型隱藏式噴頭(散射可調式-15VAN)","個",48]
["4.2","RAINBIRD 1/2\"小型隱藏式噴頭(散射可調式-18VAN)","個",3]
["4.3","RAINBIRD 1/2\"小型隱藏式噴頭(散射可調式-8VAN)","個",4]
["4.4","RAINBIRD 1/2\"小型隱藏式噴頭(9SST)","個",17]
["4.5","RAINBIRD 1/2\"小型隱藏式噴頭(15SST)","個",20]
["4.6","RAINBIRD 1/2\"小型隱藏式噴頭(15RCS)","個",2]
["4.7","RAINBIRD 1/2\"小型隱藏式噴頭(15LCS)","個",2]
["4.8","RAIN BIRD 散射噴頭1800系列，18VAN噴嘴","個",4]
["4.9","4分提升管","個",100]
["4.10","6分快速閥.銅材質(含Key.萬向角閥.高壓管5M.瞄子) ","個",4]
["4.11","6\"圓形HDPE快速閥箱","個",4]
["4.12","6分銅閘閥","個",4]
["4.13","2吋PVC主幹水管，管厚4mm","M",192]
["4.14","2吋PVC水管，管厚4mm","M",290]
["4.15","1/2吋PVC水管，管厚3mm","M",118]
["4.16","2\"-24VAC電磁閥","只",12]
["4.17","12\"矩形HDPE電磁閥箱","只",12]
["4.18","防水接頭","只",24]
["4.19","銅製閘閥-2\"-牙口式-10K","只",12]
["4.20","恆壓變頻泵站,5HP,出水量320L/min,最大揚程45M,出水口徑2\"","台",1]
["4.21","訊號線(含PVC管)","M",1851.7]
["4.22","雨水感知器","台",1]
["4.23","智能噴灌全自動控制器12站","台",1]
["4.24","2\"Y型過濾器","個",1]
["4.25","噴灌控制箱","座",1]
["4.26","雨水離心過濾器DN150*100*150","個",1]
["4.27","液位控制閥","組",1]
["4.28","2\"林根不銹鋼吸水濾網","組",1]
["4.29","配管及零星工料","式",1]
["4.30","組裝工資","工",28]
["(31)","測試工資","工",10]
[null," 計"]
[5,"排水工程"]
["5.1","4\"高腳落水頭(綠色.HDPE材質)","組",57]
["5.2","4\"平面落水頭(綠色.HDPE材質)","組",33]
["5.3","4\"PVC排水管，管厚3mm","M",198]
["5.4","3\"PVC排水管，管厚3mm","M",235]
["5.5","小型集水井","座",1]
["5.6","PVC接管另料","式",1]
["5.7","組裝工資","工",15]
["5.8","管線挖掘與回填","M",150]
["5.9","管線接續工程","式",1]
["5.10","零星工料","式",1]
["5.11","排水板總高度3cm+上層不織布過濾層(60g/㎡)","M2",645]
[null,"  計"]
["6.","照明工程"]
["6.1","景觀高燈,LED 40W","盞",8]
["6.2","景觀矮燈","盞",34]
["6.3","插地投射燈","盞",3]
["6.4","照明控制箱","座",1]
["6.5","1\"PVC電管,管厚2.7mm以上","M",633]
["6.6","配管另料","式",1]
["6.7","5.5mm平方,PVC電線","M",1899]
["6.8","安裝工資","工",15]
["6.9","管線挖掘與回填","M",633]
[null," 計"]
[null,"景觀及植栽工程費用 合計(1~6)"]
[]
["十一","其他工程(漏列項目)"]

{"sheet":"標價清單 單價分析","index":1,"n_rows":1825,"n_cols":7,"rows_kept":1825,"cut":false,"hidden":false,"merged":[]}
["項次","名                稱","單位","數   量","單   價","複    價","備註"]
["一.2","全阻隔式安全圍籬，H=2.4M,30cm止水墩,警示燈及警示標誌－施工期間維護",null,null,null,null,"部分已施作"]
[null,"  30cmRC止水墩","M",1]
[null,"  臨時鋼板圍籬 H>240 t>1.0mm","M",1]
[null,"  角鐵支柱及基礎","M",1]
[null,"  鋼板圍籬面圖案噴漆","M",1]
[null,"  警示標誌","式",1]
[null,"  圍籬清潔維護費","M",1]
[null,"  夜間警示燈(含現有圍牆)","式",1]
[null,"  零星工料","式",1]
[null,"  計","M",1]
["一.3","施工圍籬綠美化－施工期間保活養護 ","M",null,null,null,"部分已施作"]
[null,"  產品，綠籬材料-盆栽植物(15~20CM)25株/M2","M2",2.1]
[null,"  產品，綠籬盆栽容器(PP,FRP等製品)","M2",2.1]
[null,"  擺設費","M2",2.1]
[null,"  安裝及運費","式",1]
[null,"  自動灑水設備(含抽水機,時控開關,配管等)","M",1]
[null,"  人工養護費","月",25]
[null,"  灑水水費","月",25]
[null,"  零星工料","式",1]
[null,"  計","M",1]
["一.4","施工圍籬，折疊式大門，8M，(含地坪混凝土鋪設)－施工期間維護","樘",1,null,null,"部分已施作"]
[null,"  臨時出入口大門>8M 含維護","樘",1]
[null,"  水泥混凝土舖面，抗壓175 kgf/cm2，t=20cm","式",1]
[null,"  零星工料","式",1]
[null,"  計","M",1]
["一.5","環境保護，沖洗設備，(臨時洗車台設備及防污設備)－施工期間維護","處",1,null,null,"部分已施作"]
[null,"  臨時鋼製洗車台格柵 >3m*8m","座",1]
[null,"  臨時排水溝含格柵蓋及貯水池","式",1]
[null,"  洗車沖水設備連配管","式",1]
[null,"  路面沖洗設備及用具","式",1]
[null,"  零星工料","式",1]
[null,"  計"]
["一.6","廠區駐地警衛保全及崗亭","處",1]
[null,"  臨時管制鋼鋁製岡哨亭(含燈具)","處",1]
[null,"  吊運及完工撤除","式",1]
[null,"  零星工料","式",1]
[null,"  計"]
["一.7","工地臨時辦公室(含水電設備及傢俱)","式",1]
[null,"  組合式臨時房屋含水電照明整理(營造提供甲方及監造10坪)","坪",50]
[null,"  (內含辦公室,辦公桌椅,人員休息室等家具"]
[null,"   附可用之網路設備,影印機,冷氣機,,甲方3人)"]
[null,"   10人會議桌椅","式",1]
[null,"  共用廁所,衛生盥洗室,休息室等設備","坪",10]
[null,"  電腦設備及作業軟體(可上網,含甲方3套)","台",6]
[null,"  文具紙張及檔案櫃等設備","式",1]
[null,"  營造施工辦公設備(含電腦設備等)","式",1]
[null,"  其他設備及零星工料","式",1]
[null,"   計"]
["一.8","工地臨時移動廁所，含日常清潔","座",1]
[null,"  活動廁所租用","式",1]
[null,"  日常清潔及定期清潔","式",1]
[null,"  零星工料","式",1]
[null,"  計"]
["一.9","工地臨時給排水,電，照明，監視設備及臨時水電費","式",1]
[null,"  臨時設施，工程用電設備，(含用電申請)，臨時電費","式",1]
[null,"  工程用水設備，(含用水申請，用水費)，臨時水費","式",1]
[null,"  臨時設施，通訊設備，(含租用費)，網路設備費","式",1]
[null,"  工程用水設備，各層臨時用水設置及搬運維護費","式",1]
[null,"  工程用電設備，各層配電盤安裝及維護費","式",1]
[null,"  工地監視系統，監控設備，設備主機，彩色攝影機","式",1]
[null,"  零星工料","式",1]
[null,"  計"]
["一.10","施工中安全防護﹑警示措施及設備費(含各種開口),消防設施","式",1]
[null,"  各層管道間開口,電梯開口等安全防護杆","式",1]
[null,"  臨時消防防設施,防感電設施","式",1]
[null,"  鋼構施工吊籃及安全網","式",1]
[null,"  施工安全母索及防護措施","式",1]
[null,"  安全宣導及教育訓練","式",1]
[null,"  零星工料","式",1]
[null,"  計"]
["一.11","環境保護，灑水設施，各項汙染物防制及設置費","式",1]
[null,"  工地揚塵灑水處理","月",30]
[null,"  工地生活垃圾及廢棄物清運","式",1]
[null,"  工也環境清理","式",1]
[null,"  零星工料","式",1]
[null,"  計"]
["一.12","營建廢棄物及垃圾運棄及吊運費","式",1]
[null,"  營建廢棄物整理及清運","式",1]
[null,"  垃圾管道設置及移除","式",1]
[null,"  零星工料","式",1]
[null,"  計"]
["一.13","施工之臨時抽排水費","式",1]
[null,"  卸水井","式",1]
[null,"  抽排水接管","式",1]
[null,"  抽水設備費","式",1]
[null,"  電力費","式",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["一.20","全區臨時照明含地下室施工照明設備","式",1]
[null,"  臨時照明設備費","式",1]
[null,"  PVC導線","式",1]
[null,"  技術工","工",12]
[null,"  搬運費(含現場小搬運)","式",1]
[null,"  設置管理及維護","式",1]
[null,"  零星工料","式",1]
[null,"  計"]
["一.22","外部施工鷹架含安全網 含斜籬","M2",1]
[null,"  鋼管門型鷹架","M2",1]
[null,"  鷹架工","工",0.04]
[null,"  安全母索","式",1]
[null,"  安全網及帆布","M2",1]
[null,"  擋板斜籬","式",1]
[null,"  拉桿及固定件","M2",1]
[null,"  鋼架平台及樓梯踏步","式",1]
[null,"  架空三角架","M2",1]
[null,"  墊板","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["一.23","室內高層及挑空區週邊工作架 >4.5M","M2"]
[null,"  鋼管門型鷹架","M2",1]
[null,"  鷹架工","工",0.03]
[null,"  安全母索","式",1]
[null,"  拉桿及固定件","M2",1]
[null,"  鋼架平台及樓梯踏步","式",1]
[null,"  架空三角架","M2",1]
[null,"  墊板","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["二.1","擋土型鋼 H300*300*10*15 @50 L=14M","支"]
[null,"  H300 租金","T",1.302]
[null,"  開挖支撐及保護，檔板，24mm","M2",4.75]
[null,"  H型鋼打拔工資","支",1]
[null,"  14M H鋼費雜費","支",1]
[null,"  零星工料","式",1]
[null,"  計"]
["二.2","擋土型鋼 H300*300*10*15 @50 L=16M","支"]
[null,"  H300 租金","T",1.488]
[null,"  開挖支撐及保護，檔板，24mm","M2",5.7]
[null,"  H型鋼打拔工資","支",1]
[null,"  16M H鋼費雜費","支",1]
[null,"  零星工料","式",1]
[null,"  計"]
["二.3","H300 中間樁 L=13(含止水板及截樁3.6M)","支"]
[null,"  H300*300型鋼中間租金 L=13M 扣截長度","支",1]
[null,"  H300*300型鋼 截樁及鋼料損耗","式",1]
[null,"  H300 型鋼 L=13m 打拔工資","支",1]
[null,"  搬運費(含現場小搬運)","式",1]
[null,"  樁頭防水板","個",1]
[null,"  零星工料","式",1]
[null,"  合計"]
["二.4","H300 中間樁 L=15(含止水板及截樁3.75M)","支"]
[null,"  H300*300型鋼中間租金 L=15M 扣截長度","支",1]
[null,"  H300*300型鋼 截樁及鋼料損耗","式",1]
[null,"  H300 型鋼 L=15m 打拔工資","支",1]
[null,"  搬運費(含現場小搬運)","式",1]
[null,"  樁頭防水板","個",1]
[null,"  零星工料","式",1]
[null,"  合計"]
["二.5","第一層H型鋼橫擋及支撐 H-350*350*12*19 含H350圍令","M2"]
[null,"  H350 安全支撐鋼料租金","M2",1]
[null,"  H350 圍令安裝","M2",1]
[null,"  H350 水平支撐安裝","M2",1]
[null,"  H250 斜撐安裝","M2",1]
[null,"  千斤頂箱用費","M2",1]
[null,"  接頭混凝土灌築","M2",1]
[null,"  撗擋及圍令斜撐拆除","M2",1]
[null,"  鋼支撐運費","M2",1]
[null,"  零星工料","式",1]
[null,"  合計"]
["二.6","第二層H型鋼橫擋及支撐 H-400*400*13*21 含H400圍令","M2"]
[null,"  H400 安全支撐鋼料租金","M2",1]
[null,"  H400 圍令安裝","M2",1]
[null,"  H400 水平支撐安裝","M2",1]
[null,"  H300 斜撐安裝","M2",1]
[null,"  千斤頂箱用費","M2",1]
[null,"  接頭混凝土灌築","M2",1]
[null,"  撗擋及圍令斜撐拆除","M2",1]
[null,"  鋼支撐運費","M2",1]
[null,"  零星工料","式",1]
[null,"  合計"]
["二.7","第三層H型鋼橫擋回撐 H-400*400*13*21 含H400圍令","M2"]
[null,"  H400 安全支撐鋼料租金","M2",1]
[null,"  H400 圍令安裝","M2",1]
[null,"  H400 水平支撐安裝","M2",1]
[null,"  H300 斜撐安裝","M2",1]
[null,"  千斤頂箱用費","M2",1]
[null,"  接頭混凝土灌築","M2",1]
[null,"  撗擋及圍令斜撐拆除","M2",1]
[null,"  鋼支撐運費","M2",1]
[null,"  零星工料","式",1]
[null,"  合計"]
["二.8","施工輔助，施工構台","M2",1,null,null,"不作加減帳"]
[null,"  H300*300型鋼中間樁打拔及止水 L=13M","M2",1]
[null,"  H300 型鋼支撐租金","M2",1]
[null,"  覆蓋板 200*100*20CM 租金","片",0.5]
[null,"  三角拖架,小五金及另料","式",1]
[null,"  吊車施工及機具材料搬運費","M2",1]
[null,"  安全支撐組立","M2",1]
[null,"  安全欄杆","M",0.15]
[null,"  零星工料","式",1]
[null,"  計","M2",1]
["二.10","挖方(含警衛室)(依結構示意高程)","M3",1]
[null,"  挖土機及作業手","M3",1]
[null,"  機械操作手","M3",1]
[null,"  人工整平及結構物清潔","M3",1]
[null,"  零星工料","式",1]
[null,"  計"]
["二.11","廢方運棄及土方處理費(含警衛室)","M3",1,null,null,"鬆方計"]
[null,"  傾卸卡車","M3",1.2]
[null,"  司機","M3",1.2]
[null,"  小工","M3",1.2]
[null,"  土資場處理費(含証明)","M3",1.2]
[null,"  零星工料","式",1]
[null,"  計"]
["二.12","現地土方回填(含警衛室)","M3",1]
[null,"  回填及夯實工資","M3",1]
[null,"  挖土機及作業手","M3",1]
[null,"  夯實機","M3",1]
[null,"  零星工料","式",1]
[null,"  計"]
["二.13","安全監測系統","式"]
[null,"  傾斜儀 L=14,16 電子式","處",8]
[null,"  建物傾斜計","處",6]
[null,"  支撐應變計 (振弦式)","組",2]
[null,"  水位觀測井 L=12M","處",2]
[null,"  沉陷觀測釘","處",40]
[null,"  中間柱隆起桿","處",72]
[null,"  觀測記錄,報告及建議","式",1]
[null,"  儀器安裝及拆除","式",1]
[null,"  零星工料","式",1]
[null,"  計"]
["三.1","施工測量，放樣(結構建築)","M2",1]
[null,"  木料損耗","才",0.2]
[null,"  木工","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["三.2","結構用混凝土 140kgf/cm2","M3",1]
[null,"  140kg/cm2 預拌混凝土","M3",1]
[null,"  泵浦及輸送管","M3",1]
[null,"  搗築工資","M3",1]
[null,"  零星工料","式",1]
[null,"  計"]
["三.3","結構用混凝土 280kgf/cm2","M3",1]
[null,"  280kg/cm2 預拌混凝土","M3",1,null,null,"台泥,亞泥"]
[null,"  泵浦及輸送管","M3",1]
[null,"  搗築工資","M3",1]
[null,"  零星工料","式",1]
[null,"  計"]
["三.4","結構用混凝土 350kgf/cm3","M3",1]
[null,"  350kg/cm2 預拌混凝土","M3",1,null,null,"台泥,亞泥"]
[null,"  泵浦及輸送管","M3",1]
[null,"  搗築工資","M3",1]
[null,"  零星工料","式",1]
[null,"  計"]
["三.5","筏基內回填低強度混凝土","M3",1]
[null,"  低強度混凝土(控制混凝土)","M3",1]
[null,"  泵浦及輸送管","M3",1]
[null,"  搗築工資","M3",1]
[null,"  零星工料","式",1]
[null,"  計"]
["三.6","鋼筋，SD420W","噸",1]
[null,"  4200kg/cm2 鋼筋(含運費)","公噸",1.03,null,null,"豐興,東和"]
[null,"  彎紮工(含小搬運)","公噸",1]
[null,"  鐵絲","公斤",4]
[null,"  零星工料","式",1]
[null,"  計"]
["三.7","鋼絲網10*8/100*100&10*10/100*100","T",1]
[null,"  鋼筋網含運費(運至工地)","T",1]
[null,"  吊運及安裝舖設(含小搬運)","T",1]
[null,"  補強吊筋","式",1]
[null,"  零星工料","式",1]
[null,"  計"]
["三.8","普通模板","M2",1]
[null,"  普通模板板料損耗","才",1.25]
[null,"  木料支撐損耗","才",1]
[null,"  木工工資","M2",1]
[null,"  鐵絲及洋釘","公斤",0.2]
[null,"  零星工料","式",1]
[null,"  計"]
["三.9","平頂清水模板(含獨立樑柱側)","M2",1]
[null,"  夾板模板板料損耗","才",1.25]
[null,"  木料支撐損耗","才",1]
[null,"  木工工資","M2",1]
[null,"  鐵絲及洋釘","公斤",0.2]
[null,"  零星工料","式",1]
[null,"  計"]
["三.10","閉口型鋼承板 高65*1.2","M2",1]
[null,"  鍍鋅鋼承板，閉口型，H65 1.2mm含運費","M2",1]
[null,"  承板端收邊鋼板","M2",1,null,null,"平均分攤"]
[null,"  鋼承板安裝","M2",1]
[null,"  開孔及補強含樓板尾端","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["四.1","鋼板焊接口型鋼 SN490B","T",1]
[null,"   鋼板 SN-490B","公噸",1.05]
[null,"  廠製加工(含製造圖,剪裁,機械加工,成型,校正等)","公噸",1]
[null,"  鋼構加工材料(含焊條,氫氧氣,乙炔及其他)","公噸",1]
[null,"  鋼料噴吵除銹","公噸",1]
[null,"  鋼料小搬運費","公噸",1]
[null,"  零星工料","式",1]
[null,"  計"]
["四.2","BH及RH型鋼 SN490B","T",1]
[null,"    RH型鋼 SN-490B,BH型鋼 SN-490B","公噸",1.05]
[null,"  廠製加工(含製造圖,剪裁,機械加工,成型,校正等)","公噸",1]
[null,"  鋼構加工材料(含焊條,氫氧氣,乙炔及其他)","公噸",1]
[null,"  鋼料噴吵除銹","公噸",1]
[null,"  鋼料小搬運費","公噸",1]
[null,"  零星工料","式",1]
[null,"  計"]
["四.3","H型鋼 A572","T",1]
[null,"  RH型鋼 A572","公噸",1.05]
[null,"  廠製加工(含製造圖,剪裁,機械加工,成型,校正等)","公噸",1]
[null,"  鋼構加工材料(含焊條,氫氧氣,乙炔及其他)","公噸",1]
[null,"  鋼料噴吵除銹","公噸",1]
[null,"  鋼料小搬運費","公噸",1]
[null,"  零星工料","式",1]
[null,"  計"]
["四.4","H型鋼 A36","T",1]
[null,"  RH型鋼 A36","公噸",1.05]
[null,"  廠製加工(含製造圖,剪裁,機械加工,成型,校正等)","公噸",1]
[null,"  鋼構加工材料(含焊條,氫氧氣,乙炔及其他)","公噸",1]
[null,"  鋼料噴吵除銹","公噸",1]
[null,"  鋼料小搬運費","公噸",1]
[null,"  零星工料","式",1]
[null,"  計"]
["四.5","鋼板 SN490B,A572","T",1]
[null,"  鋼板  SN-490B","公噸",1.05]
[null,"  廠製加工(含製造圖,剪裁,機械加工,成型,校正等)","公噸",1]
[null,"  鋼構加工材料(含焊條,氫氧氣,乙炔及其他)","公噸",1]
[null,"  鋼料噴吵除銹","公噸",1]
[null,"  鋼料小搬運費","公噸",1]
[null,"  零星工料","式",1]
[null,"  計"]
["四.6","鋼板 A36","T",1]
[null,"  鋼板  A36","公噸",1.05]
[null,"  廠製加工(含製造圖,剪裁,機械加工,成型,校正等)","公噸",1]
[null,"  鋼構加工材料(含焊條,氫氧氣,乙炔及其他)","公噸",1]
[null,"  鋼料噴吵除銹","公噸",1]
[null,"  鋼料小搬運費","公噸",1]
[null,"  零星工料","式",1]
[null,"  計"]
[]
["五.1","外牆造型2.5mm氟碳烤漆鋁包板牆(含雨遮及各種飾板)","M2",1]
[null,"  熱浸鍍鋅鋼構件","M2",1]
[null,"  2.5mm氟碳烤漆鋁板","M2",1.1000000000000001]
[null,"  鋁板加工","M2",1]
[null,"  隔熱岩棉+鋁箔","M2",1]
[null,"  無污染矽膠防水填縫+泡棉+五金配件","M2",1]
[null,"  包裝運輸","M2",1]
[null,"  帷幕安裝費","M2",1]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["五.2","外牆4mm氟碳烤漆鋁複合板包板牆","M2",1]
[null,"  熱浸鍍鋅鋼構件","M2",1]
[null,"  4mm氟碳烤漆鋁複合板","M2",1.05]
[null,"  鋁複合板加工","M2",1]
[null,"  隔熱岩棉+鋁箔","M2",1]
[null,"  無污染矽膠防水填縫+泡棉+五金配件","M2",1]
[null,"  包裝運輸","M2",1]
[null,"  帷幕安裝費","M2",1]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["五.3","防火層間塞","M",1]
[null,"  層間填塞鋼板","M",1]
[null,"  防火岩棉板填塞","M",1]
[null,"  防火塗料","M",1]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["五a","1:3水泥砂漿","M3",1]
[null,"  水泥","包",9]
[null,"  砂","M3",0.95]
[null,"  拌合技術工","工",0.28000000000000003]
[null,"  零星工料","式",1]
[null,"  計"]
["五b","1:2防水水泥砂漿","M3",1]
[null,"  水泥","包",13]
[null,"  砂","M3",0.94]
[null,"  拌合技術工","工",0.28000000000000003]
[null,"  零星工料","式",1]
[null,"  計"]
["五.4","外牆貼45mm*45mm小口磚","M2",1]
[null,"  1:2防水水泥砂漿","M3",0.02]
[null,"  防水劑 ","公斤",0.3]
[null,"  小口釉面磚 4.5*4.5","才",11]
[null,"  磁磚乳膠黏著劑 ","M2",1]
[null,"  磁磚嵌縫劑 ","M2",1]
[null,"  工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["五.5","警衛室窗台板貼花崗石","M2",1]
[null,"  1:3水泥砂漿","M3",0.02]
[null,"  牆面粉刷整平","M2",1]
[null,"  石材乳膠黏著劑","M2",1]
[null,"  3cm花崗石材含6面防護及磨邊","才",11]
[null,"  背面加工加不銹鋼線","M2",1]
[null,"  RC牆面鋼釘固定","M2",1]
[null,"  石材安裝工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["五.6","氟碳烤漆金屬格柵裝飾牆","M2",1]
[null,"  氟碳烤漆格柵(含端口收邊蓋板)","M2",1]
[null,"  熱浸鍍鋅橫桿及補強另件","M2",1]
[null,"  鋁格柵安裝及清潔 ","M2",1]
[null,"  無污染矽膠防水填縫","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["五.7","氣體區氟碳烤漆金屬格柵牆","M2",1]
[null,"  氣體區氟碳烤漆格柵(含端口收邊蓋板)","M2",1]
[null,"  固定不銹鋼鐵件、基礎及五金配件","式",1]
[null,"  無收縮水泥填縫","式",1]
[null,"  鋁格柵安裝及清潔 ","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["五.8","氣體區氟碳烤漆不銹鋼單片橫拉門 125*226","樘",1]
[null,"  氣體區氟碳烤漆不銹鋼單片橫拉門 125*226(本體、框料及配件)","M2",2.8249999999999997]
[null,"  安裝及清潔 ","M2",2.8249999999999997]
[null,"  不銹鋼門扣及三段鎖","組",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.1","高層纖維水泥板灌漿隔間","M2",1]
[null,"  18GA C型輕鋼架組合","M2",1]
[null,"  12m纖維水泥板","M2",2.2000000000000002]
[null,"  輕質灌漿材","M2",1]
[null,"  施工費","M2",1]
[null,"  貼纖維布及批土填縫","M2",2]
[null,"  小五金及小搬運","M2",2]
[null,"  零星工料","式",1]
[null,"  計"]
["六.2","一般樓層纖維水泥板灌漿隔間","M2",1]
[null,"  20GA C型輕鋼架組合","M2",1]
[null,"  12m纖維水泥板","M2",2.2000000000000002]
[null,"  輕質灌漿材","M2",1]
[null,"  施工費","M2",1]
[null,"  貼纖維布及批土填縫","M2",2]
[null,"  小五金及小搬運","M2",2]
[null,"  零星工料","式",1]
[null,"  計"]
["六.3","纖維水泥板廁所外側單面封板","M2",1]
[null,"  20GA C型輕鋼架組合","M2",1]
[null,"  12m纖維水泥板","M2",1.1000000000000001]
[null,"  施工費","M2",1]
[null,"  貼纖維布及批土填縫","M2",1]
[null,"  小五金及小搬運","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.4","高層雙面矽酸鈣板防火隔間牆","M2",1]
[null,"  18GA C型輕鋼架組合","M2",1]
[null,"  12mm 矽酸鈣板 無煙毒板","M2",2.2000000000000002]
[null,"  2\" 60K防火岩棉","M2",1]
[null,"  施工費","M2",1]
[null,"  貼纖維布及批土填縫","M2",2]
[null,"  小五金及小搬運","M2",2]
[null,"  零星工料","式",1]
[null,"  計"]
["六.5","一般樓層雙面矽酸鈣板防火隔間牆","M2",1]
[null,"  20GA C型輕鋼架組合","M2",1]
[null,"  12mm 矽酸鈣板 無煙毒板","M2",2.2000000000000002]
[null,"  2\" 60K防火岩棉","M2",1]
[null,"  施工費","M2",1]
[null,"  貼纖維布及批土填縫","M2",2]
[null,"  小五金及小搬運","M2",2]
[null,"  零星工料","式",1]
[null,"  計"]
["六.6","鋁帷幕牆內側單面封牆","M3",1]
[null,"  20GA C型輕鋼架組合","M2",1]
[null,"  9mm 矽酸鈣板 無煙毒板","M2",1.1000000000000001]
[null,"  2\" 60K防火岩棉","M2",1]
[null,"  施工費","M2",1]
[null,"  貼纖維布及批土填縫","M2",1]
[null,"  小五金及小搬運","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.7","外牆內側金屬庫板隔間牆","M2",1]
[null,"  50mm厚鋼板庫板(內夾岩棉板)","M2",1]
[null,"  組合及收邊輕鋼骨架","M2",1]
[null,"  施工費","M2",1]
[null,"  填縫及收邊","M2",1]
[null,"  小五金及小搬運","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.8","一小時防火時效金屬庫板牆(挑空區管道間)","M2",1]
[null,"  組合輕鋼架","M2",1]
[null,"  50mm厚鋼板庫板(內夾岩棉板)","M2",1.1000000000000001]
[null,"  施工費","M2",1]
[null,"  填縫及收邊","M2",1]
[null,"  小五金及小搬運","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.9","牆面1:3水泥粉刷","M2",1]
[null,"  1:3水泥砂漿","M3",0.02]
[null,"  泥工工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.11","牆面1:3水泥粉刷批土刷水泥漆","M2",1]
[null,"  1:3水泥砂漿","M3",0.02]
[null,"  泥工工資","M2",1]
[null,"  表面批土","M2",1]
[null,"  水性水泥漆工料","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.12","地下室外側牆面1:2防水泥粉刷刷水泥漆","M2",1]
[null,"  1:2防水水泥砂漿","M3",0.02]
[null,"  防水劑 ","公斤",0.3]
[null,"  泥工工資","M2",1]
[null,"  表面批土","M2",1]
[null,"  水性水泥漆工料","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.13","輕隔間牆面批土刷水泥漆","M2",1]
[null,"  輕隔間板表面填縫批土","M2",1]
[null,"  接縫AB膠填縫及不織布黏著","M2",1]
[null,"  水性水泥漆工料","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.14","輕隔間牆面補強乾式吊掛石材","M2",1]
[null,"  輕隔間牆骨架鋼板補強","M2",1]
[null,"  2cm花崗石材(含六面防護及磨邊)","才",11]
[null,"  背擴孔加工及螺栓","M2",1]
[null,"  二次鐵件安裝","M2",1]
[null,"  石材安裝工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.15","RC牆面乾掛石材","M2",1]
[null,"  RC牆面水泥批平","M2",1]
[null,"  2cm花崗石材(含六面防護及磨邊)","才",11]
[null,"  背擴孔加工及螺栓","M2",1]
[null,"  二次鐵件安裝","M2",1]
[null,"  石材安裝工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.16","廁所牆面1:2水泥砂漿貼30*60磁磚","M2",1]
[null,"  1:2水泥砂漿","M3",0.02]
[null,"  泥工粉平工資","M2",1]
[null,"  30*60面磚 ","塊",5.6]
[null,"  磁磚乳膠黏著劑 ","M2",1]
[null,"  磁磚嵌縫劑 ","M2",1]
[null,"  工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.17","廁所輕隔間牆面黏著劑貼30*60磁磚","M2",1]
[null,"  輕隔間牆面全面批土整平","M2",1]
[null,"  30*60面磚 ","塊",5.6]
[null,"  磁磚乳膠黏著劑 ","M2",1]
[null,"  磁磚嵌縫劑 ","M2",1]
[null,"  工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.18","廁所牆面150CM高防水塗佈","M2",1]
[null,"  牆面表面清潔","M2",1]
[null,"  高分子複合水泥基防水材","公斤",2]
[null,"  抗裂纖維","M2",1]
[null,"  工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.19","牆面無毒防水劑+防水粉刷貼20*20面磚","M2",1]
[null,"  1:2水泥砂漿","M3",0.02]
[null,"  泥工粉平工資","M2",1]
[null,"  無毒高分子複合水泥基防水劑","公斤",2.5]
[null,"  20*20面磚 ","塊",25]
[null,"  磁磚乳膠黏著劑 ","M2",1]
[null,"  磁磚嵌縫劑 ","M2",1]
[null,"  工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.20","踢腳水泥粉刷水泥漆,10CM","M",1]
[null,"  1:3水泥砂漿","M3",2E-3]
[null,"  泥工工資","M",1]
[null,"  表面批土","M2",1]
[null,"  水性水泥漆工料","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.23","地坪乾式打底貼拋光面石材","M2",1]
[null,"  地坪高平整拍漿粉光","M2",1]
[null,"  1:3水泥砂漿","M3",0.02]
[null,"  石材乳膠黏著劑","M2",1]
[null,"  3cm花崗石材(含石材加工,六面防護及磨邊)","才",11]
[null,"  石材安裝工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.24","地坪1:3水泥砂漿貼60*60抛光石英磚","M2",1]
[null,"  地坪高平整拍漿粉光","M2",1]
[null,"  1:3水泥砂漿","M3",0.02]
[null,"  底層塗(高分子)水泥基防水材","公斤",2.5]
[null,"  60*60 拋光石英磚","塊",2.8]
[null,"  磁磚乳膠黏著劑 ","M2",1]
[null,"  磁磚嵌縫劑 ","M2",1]
[null,"  工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.25","地坪高平整拍漿粉光耐磨型環氧樹脂地坪,厚度3mm","M2",1]
[null,"  地坪高平整拍漿粉光","M2",1]
[null,"  環氧樹脂底漆","M2",1]
[null,"  2mm耐磨型加石英砂環氧樹脂中塗漆","M2",1]
[null,"  環氧樹脂面漆","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.26","斜車道整體粉光止滑型環氧樹脂,厚度5mm","M2",1]
[null,"  地坪體整順向斜坡拍漿粉光","M2",1]
[null,"  環氧樹脂底漆","M2",1]
[null,"  4mm止滑耐磨型加金鋼砂環氧樹脂中塗漆","M2",1]
[null,"  環氧樹脂面漆","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.27","地坪高平整拍漿粉光平滑型環氧樹脂地坪,厚度3mm","M2",1]
[null,"  地坪高平整拍漿粉光","M2",1]
[null,"  環氧樹脂底漆","M2",1]
[null,"  2mm自流展平滑型加石英砂環氧樹脂中塗漆","M2",1]
[null,"  環氧樹脂面漆","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.28","樓梯面貼20*20面磚+止滑磚 ","M2",1]
[null,"  1:3水泥砂漿","M3",0.02]
[null,"  20*20石英止滑磚","片",23]
[null,"  20*6樓梯石英止滑磚","片",6]
[null,"  磁磚乳膠黏著劑 ","M2",1]
[null,"  磁磚嵌縫劑 ","M2",1]
[null,"  樓梯面貼磚工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.29","樓梯面貼PVC地磚+止滑條","M2",1]
[null,"  鋼樓梯面地坪整體拍漿粉平","M2",1]
[null,"  30*30 PVC透心地磚","M2",1]
[null,"  踏步端 5CM PVC止滑條","M2",1]
[null,"  PVC地磚秥著劑","M2",1]
[null,"  樓梯面貼磚工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.30","廁所地坪防水塗佈後貼30*30止滑石英磚","M2",1]
[null,"  1:2水泥砂漿","M3",0.02]
[null,"  泥工粉平工資","M2",1]
[null,"  高分子複合水泥基防水劑","公斤",2]
[null,"  30*30止滑石英磚","塊",11]
[null,"  磁磚乳膠黏著劑 ","M2",1]
[null,"  磁磚嵌縫劑 ","M2",1]
[null,"  工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.31","無毒防水劑+1:2防水粉刷貼20*20地磚 ","M2",1]
[null,"  1:2水泥砂漿","M3",0.02]
[null,"  泥工粉平工資","M2",1]
[null,"  無毒高分子複合水泥基防水劑","公斤",2]
[null,"  20*20面磚 ","塊",25]
[null,"  磁磚乳膠黏著劑 ","M2",1]
[null,"  磁磚嵌縫劑 ","M2",1]
[null,"  工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.32","地坪高平整整體粉光","M2",1]
[null,"  標高器基準點@1M～1.5M","式",1]
[null,"  軌道或雷射工法RC灌漿補助工資","M2",1]
[null,"  車座式拍漿機整平拍漿粉光","M2",1]
[null,"  人工補助施工費","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.33","樓梯地坪收邊抿石子","M2",1]
[null,"  1:3水泥砂漿","M3",0.02]
[null,"  一分石粒","公斤",12]
[null,"  水泥","包",0.12]
[null,"  泥工抿石子工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.34","高平整整體粉光加自平泥面貼60*60cmPVC透心地磚","M2",1]
[null,"  地坪高平整拍漿粉光","M2",1]
[null,"  地坪清潔及受損修補","M3",1]
[null,"  自平泥","M2",1]
[null,"  60*60 PVC透心地磚，厚度2.5mm以上","M2",1.1000000000000001]
[null,"  PVC 地磚舖設工資(含地板膠等)","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.36","平頂清水模面噴水泥漆","M2",1]
[null,"  清水模面(含接縫)整平","M2",1]
[null,"  噴水泥漆工料(水性或油性)","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.37","平頂樑底樑側清水模面噴水泥漆 C1A","M2",1]
[null,"  樑底樑側清水模面(含接縫)整平,釘子固定螺切除磨平","M2",1]
[null,"  噴水泥漆工料(水性或油性)","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.38","平頂水泥粉刷水泥漆(含樑底樑側)","M2",1]
[null,"  1:3水泥砂漿","M3",0.02]
[null,"  泥工工資","M2",1]
[null,"  表面批土","M2",1]
[null,"  水性水泥漆工料","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.39","鋼樓梯背板噴漆(含側板)","M2",1]
[null,"  鋼板面清潔","M2",1]
[null,"  底漆噴塗","M2",1]
[null,"  面漆噴塗","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.40","樓電梯位置磚","M2",1]
[null,"  位置磚地坪整平","M2",1]
[null,"  位置磚(30*30)石英磚或花崗磚(表面顆粒狀","M2",1]
[null,"  磁磚乳膠黏著劑 ","M2",1]
[null,"  磁磚嵌縫劑 ","M2",1]
[null,"  位置面貼磚工資,表面齊平相鄰地坪","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.41","筏基內水池地坪牆面加七厘石防水粉刷","M2",1]
[null,"  高分子複合水泥基防水劑","公斤",2]
[null,"  1:2水泥砂漿","M3",0.02]
[null,"  防水劑 ","公斤",0.3]
[null,"  泥工粉平工資(含七厘石)","M2",1]
[null,"  七厘石粒","公斤",12]
[null,"  水泥","包",0.12]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.42","筏基空調及製程水池地坪牆面防水粉刷貼20*20面磚","M2",1]
[null,"  1:2水泥砂漿","M3",0.02]
[null,"  防水劑 ","公斤",0.3]
[null,"  泥工粉平工資","M2",1]
[null,"  20*20面磚 ","塊",25]
[null,"  磁磚乳膠黏著劑 ","M2",1]
[null,"  磁磚嵌縫劑 ","M2",1]
[null,"  工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.43","屋面及露台防水隔熱層","M2",1]
[null,"  地坪整體拍漿粉光","M2",1]
[null,"  地坪清潔","M2",1]
[null,"  底油(Primer 0.2kg/M2)","M2",1]
[null,"  彈性防水膠3.6kg/㎡","M2",1,null,null,"依材料特性施作"]
[null,"  2mm橡化瀝青自黏式防水膜 表面HDPE雙層貼合","M2",1]
[null,"  硬質聚苯乙烯PS隔熱板，厚度3.5cm+濾水布1mm","M2",1]
[null,"  牆面地坪轉角施作倒角及防水補強","M2",1]
[null,"  鋼筋網15*15*6含運費及吊裝","M2",1]
[null,"  210混凝土內加抗裂纖維網","M2",1]
[null,"  混凝土面整體拍漿粉光(依洩水面施作地度)","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.44","屋面1/2B汎水壓磚","M",1]
[null,"  地坪,牆面清潔","M",1]
[null,"  紅磚","塊",15]
[null,"  1:3水泥砂漿","M3",0.02]
[null,"  泥工工資","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.45","女兒牆內側防水粉刷(含汎水)","M2",1]
[null,"  1:3水泥砂漿","M3",0.02]
[null,"  泥工工資","M2",1]
[null,"  底油(Primer 0.2kg/M2)","M2",1]
[null,"  水泥基防水材","公斤",2.5]
[null,"  防水工資","M2",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.46","屋面防水層上隔熱磚兼淺溝","M",1]
[null,"  屋頂隔熱預留邊溝模板","M",1]
[null,"  高腳隔熱磚(長度30cm*寬度30cm*高度5.5cm)","M",1]
[null,"  舖設工資","M",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["六.47","地下室頂板防水層含保護層","M2",1]
[null,"  地坪整體拍漿粉光","M2",1]
[null,"  地坪清潔","M2",1]
[null,"  底油(Primer 0.2kg/M2)","M2",1.02]
[null,"  彈性防水膠3kg/㎡","M2",1.02,null,null,"依材料特性施作"]
[null,"  2mm橡化瀝青自黏式防水膜 表面HDPE雙層貼合","M2",1.02]
[null,"  牆面地坪轉角施作倒角及防水補強","M2",1]
[null,"  鋼筋網15*15*6含運費及吊裝","M2",1.25]
[null,"  210混凝土內加抗裂纖維網","M2",1]
[null,"  混凝土面整體拍漿粉光(依洩水面施作地度)","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.48","筏基及一層外推地坪防潮層","M2",1]
[null,"  清潔及底油塗佈","M2",1]
[null,"  1.0mmHDPE自黏式防水膜","M2",1]
[null,"  施工費","M2",1]
[null,"  接頭,收邊處理","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.49","地下室外牆接縫防水打鑿","M",1]
[null,"  牆面清潔","M",1]
[null,"  外牆工作縫接縫V型打鑿","M",1]
[null,"  樹脂砂漿填補整平","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.50","地下室外牆防水層","M2",1]
[null,"  牆面清潔","M2",1]
[null,"  牆面1:3水泥砂漿粉平","M2",1]
[null,"  底油(Primer 0.2kg/M2)","M2",1]
[null,"  橡化瀝青彈性防水膠2KG/M2","M2",1]
[null,"  水泥基防水材","公斤",2.5]
[null,"  樹脂砂漿塗佈 二道","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.51","屋面設備基座 15CM高","M2",1]
[null,"  設備基座打打混凝土 280kg/cm2","M3",0.15]
[null,"  #4鋼筋含加工綁紮","T",2.5000000000000001E-2]
[null,"  四邊模板","M2",0.15]
[null,"  面層高平整拍漿粉平","M2",1]
[null,"  零星工料","式",1]
[null,"  計"]
["六.53","屋頂女兒牆笠木蓋板收邊","M",1]
[null,"  烤漆鋁擠型骨架","M2",1.25]
[null,"  2.5mm氟碳烤漆鋁板及加工","M2",0.25]
[null,"  無污染矽膠防水填縫","M",1.25]
[null,"  包裝運輸","M2",1.25]
[null,"  安裝費","M",1]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["六.56","屋頂及露台女兒牆泛水收邊下立牆牆面防水設施"]
[null,"  牆面清潔","M2",1]
[null,"  底油(Primer 0.2kg/M2)","M2",1]
[null,"  彈性防水膠1kg/㎡","M2",1,null,null,"依材料特性施作"]
[null,"  聚脂纖維布","M2",1]
[null,"  彈性防水膠1kg/㎡","M2",1,null,null,"依材料特性施作"]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.1","D1 200*235 不銹鋼烤漆安全門 F60A (遮煙)","樘",1]
[null,"  F60A 200*235雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  順位調整器","組",1]
[null,"  防火級不銹鋼平推鎖","付",1]
[null,"  不銹鋼平推副鎖+天地+防塵座","付",1]
[null,"  外側水平把手","只",2]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.2","D2 120*220 不銹鋼烤漆安全門 F60A (遮煙)","樘",1]
[null,"  F60A 120*220 鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",1]
[null,"  防火級不銹鋼平推鎖","付",1]
[null,"  外側水平把手","只",1]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.3","D3 120*220 不銹鋼烤漆安全門 F60A (遮煙)","樘",1]
[null,"  F60A 120*220 鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級旗型鉸鏈 4.5\"*4.6mm 4培林","片",4]
[null,"  防火級門弓器(可調式)","組",1]
[null,"  防火級不銹鋼平推鎖","付",1]
[null,"  外側水平把手","只",1]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.4","D4 250*250 不銹鋼烤漆防火門 F60A (遮煙)","樘",1]
[null,"  F60A 250*250雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  不銹鋼副鎖+水平把手","付",1]
[null,"  防火級天地栓+防塵座","付",1]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.5","D5 240*220 不銹鋼烤漆防火門 F60A (遮煙)","樘",1]
[null,"  F60A 240*220雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  不銹鋼副鎖+水平把手","付",1]
[null,"  防火級天地栓+防塵座","付",1]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.6","D6 240*220 不銹鋼烤漆防火門 F60A (遮煙)","樘",1]
[null,"  F60A 240*220雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  不銹鋼副鎖+水平把手","付",1]
[null,"  防火級天地栓+防塵座","付",1]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.7","D7 200*235 不銹鋼烤漆安全門 F60A (遮煙)","樘",1]
[null,"  F60A 200*235雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  防火級門弓器(可調式)","組",2]
[null,"  防火級不銹鋼平推鎖","付",1]
[null,"  不銹鋼平推副鎖+天地+防塵座","付",1]
[null,"  外側水平把手","只",2]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.8","D8 200*220 不銹鋼烤漆防火門 F60A (遮煙)","樘",1]
[null,"  F60A 200*220雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  不銹鋼副鎖+水平把手","付",1]
[null,"  防火級天地栓+防塵座","付",1]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.9","D9 120*220 不銹鋼烤漆防火門 F60A (遮煙)","樘",1]
[null,"  F60A 120*220 鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",1]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.10","D10 100*220 不銹鋼烤漆防火門 F60A (遮煙)","樘",1]
[null,"  F60A 100*220 鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",1]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.11","D11 160*210 不銹鋼烤漆防火門 F60A (遮煙)","樘",1]
[null,"  F60A 160*210雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  不銹鋼副鎖+水平把手","付",1]
[null,"  防火級天地栓+防塵座","付",1]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.12","D12 160*200 不銹鋼烤漆防火門 F60A (遮煙)","樘",1]
[null,"  F60A 160*200雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  不銹鋼副鎖+水平把手","付",1]
[null,"  防火級天地栓+防塵座","付",1]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.13","D13 90*210 不銹鋼烤漆防火門 F60A (遮煙)","樘",1]
[null,"  F60A 90*210 鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",1]
[null,"  防火級不銹鋼平推鎖","付",1]
[null,"  外側水平把手","只",1]
[null,"  遮煙裝置(氣密條+下降壓條)","只",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.14","D14 300*300 不銹鋼烤漆防火門 F60A","樘",1]
[null,"  F60A 300*300雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  不銹鋼副鎖+水平把手","付",1]
[null,"  防火級天地栓+防塵座","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.15","D15 250*250 不銹鋼烤漆防火門 F60A","樘",1]
[null,"  F60A 250*250雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  不銹鋼副鎖+水平把手","付",1]
[null,"  防火級天地栓+防塵座","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.16","D16 240*220 不銹鋼烤漆防火門 F60A","樘",1]
[null,"  F60A 240*220雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  不銹鋼副鎖+水平把手","付",1]
[null,"  防火級天地栓+防塵座","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.17","D17 200*220 不銹鋼烤漆防火門 F60A","樘",1]
[null,"  F60A 200*220雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",2]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  不銹鋼副鎖+水平把手","付",1]
[null,"  防火級天地栓+防塵座","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.18","D18 120*220 不銹鋼烤漆防火門 F60A","樘",1]
[null,"  F60A 120*220 鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",1]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.19","D19 100*220 不銹鋼烤漆防火門 F60A","樘",1]
[null,"  F60A 100*220 鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級地鉸鏈","組",1]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.20","D20 200*220 不銹鋼烤漆門 ","樘",1]
[null,"  F60A 200*220雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級旗型鉸鏈 4.5\"*4.6mm 4培林","片",8]
[null,"  防火級門弓器(可調式)","組",2]
[null,"  防火級不銹鋼匣式鎖連水平把手","付",1]
[null,"  不銹鋼副鎖+水平把手","付",1]
[null,"  防火級天地栓+防塵座","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.21","D21 120*220 不銹鋼烤漆門","樘",1]
[null,"  120*220 鋼板烤漆門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  地鉸鏈","組",1]
[null,"  不銹鋼匣式鎖連水平把手","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.22","D22 120*220 不銹鋼烤漆門","樘",1]
[null,"  120*220 鋼板烤漆門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級旗型鉸鏈 4.5\"*4.6mm 4培林","片",4]
[null,"  防火級門弓器(可調式)","組",1]
[null,"  不銹鋼匣式鎖連水平把手","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.23","D23 100*220 鋼製烤漆門 含視窗","樘",1]
[null,"  100*220 鋼板烤漆門(含門框)","樘",1]
[null,"  視窗含玻璃 20*150","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  旗型鉸鏈 4.5\"*4.6mm 4培林","片",3]
[null,"  不銹鋼輔助鎖+水平把手","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.24","D24 90*220 鋼製烤漆門 含視窗","樘",1]
[null,"  90*220 鋼板烤漆門(含門框)","樘",1]
[null,"  視窗含玻璃 20*150","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  旗型鉸鏈 4.5\"*4.6mm 4培林","片",3]
[null,"  不銹鋼輔助鎖+水平把手","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.25","D25 80*210 鋼製烤漆門 含百葉","樘",1]
[null,"  80*220 鋼板烤漆門(含門框)","樘",1]
[null,"  烤漆百葉窗","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  旗型鉸鏈 4.5\"*4.6mm 4培林","片",3]
[null,"  不銹鋼輔助鎖+水平把手","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.26","D26 200*205 不銹鋼烤漆門 台電規格橫拉門 ","樘",1]
[null,"  200*205台電配電室標準橫拉門","樘",1]
[null,"  安裝工料","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.27","D27 110*210 SMC 無障礙拉門","樘",1]
[null,"  SMC 門扇 110*210 (含塑鋼百葉,標示牌)","扇",1]
[null,"  橫拉門吊軌組半自動門機","組",1]
[null,"  不銹鋼指示鎖含把手","付",1]
[null,"  安裝工料","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.28","D28 120*120 不銹鋼防火維修門 F60B","樘",1]
[null,"  F60B 120*120 雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級旗型鉸鏈 3.5\"*3mm 4培林","片",4]
[null,"  防火級不銹鋼平頭鎖","付",1]
[null,"  不銹鋼凹槽把手","付",2]
[null,"  零星工料","式",1]
[null,"  計"]
["七.29","D29 80*120 不銹鋼防火維修門 F60B","樘",1]
[null,"  F60B 80*120 雙開鋼板烤漆防火門(含門框)","樘",1]
[null,"  安裝及填縫","樘",1]
[null,"  防火級旗型鉸鏈 3.5\"*3mm 4培林","片",2]
[null,"  防火級不銹鋼平頭鎖","付",1]
[null,"  不銹鋼凹槽把手","付",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.30","SD1  700*322  不銹鋼電動捲門","樘",1]
[null,"  不銹鋼板捲門片","M2",26.040000000000003]
[null,"  開閉機 2HP","組",1]
[null,"  捲軸鐵件及座板固定件","M",7]
[null,"  防風鉤","組",1]
[null,"  內外控制開關及開關盒","組",1]
[null,"  不銹鋼門箱","M",7]
[null,"  不銹鋼門軌","M",6.44]
[null,"  不銹鋼底座","M",7]
[null,"  安裝及小搬運","M2",26.04]
[null,"  障礙感知器連主機(含配線)","M",7]
[null,"  防壓主機","組",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["七.31","SD2  310*445  不銹鋼電動捲門","樘",1]
[null,"  不銹鋼板捲門片","M2",15.5]
[null,"  開閉機 1HP","組",1]
[null,"  捲軸鐵件及座板固定件","M",3.1]
[null,"  防風鉤","組",1]
[null,"  內外控制開關及開關盒","組",1]
[null,"  不銹鋼門箱","M",3.1]
[null,"  不銹鋼門軌","M",8.9]
[null,"  不銹鋼底座","M",3.1]
[null,"  安裝及小搬運","M2",15.5]
[null,"  障礙感知器連主機(含配線)","M",3.1]
[null,"  防壓主機","組",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["七.32","SD3  350*400  不銹鋼電動捲門","樘",1]
[null,"  不銹鋼板捲門片","M2",15.75]
[null,"  開閉機 1HP","組",1]
[null,"  捲軸鐵件及座板固定件","M",3.5]
[null,"  防風鉤","組",1]
[null,"  內外控制開關及開關盒","組",1]
[null,"  不銹鋼門箱","M",3.5]
[null,"  不銹鋼門軌","M",8]
[null,"  不銹鋼底座","M",3.5]
[null,"  安裝及小搬運","M2",15.75]
[null,"  障礙感知器連主機(含配線)","M",3.5]
[null,"  防壓主機","組",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["七.33","SD4  350*375  不銹鋼電動捲門","樘",1]
[null,"  不銹鋼板捲門片","M2",14.875]
[null,"  開閉機 1HP","組",1]
[null,"  捲軸鐵件及座板固定件","M",3.5]
[null,"  防風鉤","組",1]
[null,"  內外控制開關及開關盒","組",1]
[null,"  不銹鋼門箱","M",3.5]
[null,"  不銹鋼門軌","M",7.5]
[null,"  不銹鋼底座","M",3.5]
[null,"  安裝及小搬運","M2",14.9]
[null,"  障礙感知器連主機(含配線)","M",3.5]
[null,"  防壓主機","組",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["七.34","SD5  500*280  不銹鋼電動防火捲門 60A","樘",1]
[null,"  不銹鋼板捲門片","M2",16]
[null,"  開閉機 1HP","組",1]
[null,"  捲軸鐵件及座板固定件","M",5]
[null,"  防風鉤","組",1]
[null,"  內外控制開關及開關盒","組",1]
[null,"  不銹鋼門箱","M",5]
[null,"  不銹鋼門軌","M",5.6]
[null,"  不銹鋼底座","M",5]
[null,"  安裝及小搬運","M2",16]
[null,"  障礙感知器連主機(含配線)","M",3.5]
[null,"  防壓主機","組",1]
[null,"  工具損耗","式",1]
[null,"  計"]
["七.36","L1 鍍鋅鋼板防火百葉閘門 65*65","樘",1]
[null,"  室內型防火百葉窗","樘",1]
[null,"  窗框填縫及塞水路","M",1.4]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.37","L1a 鍍鋅鋼板防火百葉閘門 65*65","樘",1]
[null,"  室內型防火百葉窗","樘",1]
[null,"  窗框填縫及塞水路","M",1.4]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.38","L2 284*156 防颱型鋁百葉","樘",1]
[null,"  鋁質百葉窗，防颱型，氟碳烤漆(含不銹鋼防蟲網，三折式，透風率＞50.0%)","M2",4.43,null,null,"(風速22M/S,雨量200mm/hr,風吸入量3.0m3/s,阻雨率100%)"]
[null,"  防颱型鋁百葉組裝清潔(含固定五金)","M2",4.43]
[null,"  無污染Silicone 防水填縫","M",8.8000000000000007]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",8.8000000000000007]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.39","L3 134*156 防颱型鋁百葉","樘",1]
[null,"  鋁質百葉窗，防颱型，氟碳烤漆(含不銹鋼防蟲網，三折式，透風率＞50.0%)","M2",2.1,null,null,"(風速22M/S,雨量200mm/hr,風吸入量3.0m3/s,阻雨率100%)"]
[null,"  防颱型鋁百葉組裝清潔(含固定五金)","M2",2.1]
[null,"  無污染Silicone 防水填縫","M",5.8]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",5.8]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.40","L4 140*200 防颱型鋁百葉","樘",1]
[null,"  鋁質百葉窗，防颱型，氟碳烤漆(含不銹鋼防蟲網，三折式，透風率＞50.0%)","M2",2.8,null,null,"(風速22M/S,雨量200mm/hr,風吸入量3.0m3/s,阻雨率100%)"]
[null,"  防颱型鋁百葉組裝清潔(含固定五金)","M2",2.8]
[null,"  無污染Silicone 防水填縫","M",6.8]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",6.8]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.41","L5 250*100 防颱型鋁百葉","樘",1]
[null,"  鋁質百葉窗，防颱型，氟碳烤漆(含不銹鋼防蟲網，三折式，透風率＞50.0%)","M2",2.5,null,null,"(風速22M/S,雨量200mm/hr,風吸入量3.0m3/s,阻雨率100%)"]
[null,"  防颱型鋁百葉組裝清潔(含固定五金)","M2",2.5]
[null,"  無污染Silicone 防水填縫","M",7]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",7]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.42","L6 1100*100 防颱型鋁百葉+鋁窗","樘",1]
[null,"  鋁質百葉窗，防颱型，氟碳烤漆(含不銹鋼防蟲網，三折式，透風率＞50.0%)","M2",11,null,null,"(風速22M/S,雨量200mm/hr,風吸入量3.0m3/s,阻雨率100%)"]
[null,"  防颱型鋁百葉組裝清潔(含固定五金)","M2",11]
[null,"  無污染Silicone 防水填縫","M",24]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",24]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.43","L7 85*150 防颱型鋁百葉","樘",1]
[null,"  鋁質百葉窗，防颱型，氟碳烤漆(含不銹鋼防蟲網，三折式，透風率＞50.0%)","M2",1.2749999999999999,null,null,"(風速22M/S,雨量200mm/hr,風吸入量3.0m3/s,阻雨率100%)"]
[null,"  防颱型鋁百葉組裝清潔(含固定五金)","M2",1.2749999999999999]
[null,"  無污染Silicone 防水填縫","M",4.7]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",4.7]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.44","L8 100*100 可關閉防水型鋁百葉","樘",1]
[null,"  防水型活動式葉片鋁百葉含框","M2",1]
[null,"  開閉撥片連桿","M2",1]
[null,"  無污染Silicone 防水填縫","M",4]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",4]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.45","L8a 100*100 可關閉防水型鋁百葉","樘",1]
[null,"  防水型活動式葉片鋁百葉含框","M2",1]
[null,"  開閉撥片連桿","M2",1]
[null,"  無污染Silicone 防水填縫","M",4]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",4]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.46","L9 60*60 防颱型鋁百葉","樘",1]
[null,"  鋁質百葉窗，防颱型，氟碳烤漆(含不銹鋼防蟲網，三折式，透風率＞50.0%)","M2",0.36,null,null,"(風速22M/S,雨量200mm/hr,風吸入量3.0m3/s,阻雨率100%)"]
[null,"  防颱型鋁百葉組裝清潔(含固定五金)","M2",0.36]
[null,"  無污染Silicone 防水填縫","M",2.4]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",2.4]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.47","L9a 60*60 防颱型鋁百葉","樘",1]
[null,"  鋁質百葉窗，防颱型，氟碳烤漆(含不銹鋼防蟲網，三折式，透風率＞50.0%)","M2",0.36,null,null,"(風速22M/S,雨量200mm/hr,風吸入量3.0m3/s,阻雨率100%)"]
[null,"  防颱型鋁百葉組裝清潔(含固定五金)","M2",0.36]
[null,"  無污染Silicone 防水填縫","M",2.4]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",2.4]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.48","L10 130*55 防颱型鋁百葉","樘",1]
[null,"  鋁質百葉窗，防颱型，氟碳烤漆(含不銹鋼防蟲網，三折式，透風率＞50.0%)","M2",0.71499999999999997,null,null,"(風速22M/S,雨量200mm/hr,風吸入量3.0m3/s,阻雨率100%)"]
[null,"  防颱型鋁百葉組裝清潔(含固定五金)","M2",0.71499999999999997]
[null,"  無污染Silicone 防水填縫","M",3.7]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",3.7]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.49","W1 1100*200 鋁窗 (附摺疊紗窗)","樘",1]
[null,"  氟碳烤漆鋁窗","樘",1]
[null,"  推射子窗含五金","樘",6]
[null,"  摺疊紗窗","樘",6]
[null,"  8mm微反強化玻璃","才",242]
[null,"  無污染Silicone 防水填縫","M",26]
[null,"  嵌縫及塞水路，連工帶料","M",26]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.50","W2 1100*100 鋁窗 (附摺疊紗窗)","樘",1]
[null,"  氟碳烤漆鋁窗","樘",1]
[null,"  推射子窗含五金","樘",3]
[null,"  摺疊紗窗","樘",3]
[null,"  8mm微反強化玻璃","才",121]
[null,"  無污染Silicone 防水填縫","M",24]
[null,"  嵌縫及塞水路，連工帶料","M",24]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.51","W3 300*200 鋁窗 (附摺疊紗窗)","樘",1]
[null,"  氟碳烤漆鋁窗","樘",1]
[null,"  推射子窗含五金","樘",6]
[null,"  摺疊紗窗","樘",6]
[null,"  8mm微反強化玻璃","才",66]
[null,"  無污染Silicone 防水填縫","M",10]
[null,"  嵌縫及塞水路，連工帶料","M",10]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.52","W4 180*100 鋁窗 (附摺疊紗窗)","樘",1]
[null,"  氟碳烤漆鋁窗","樘",1]
[null,"  推射子窗含五金","樘",2]
[null,"  摺疊紗窗","樘",2]
[null,"  8mm微反強化玻璃","才",20]
[null,"  無污染Silicone 防水填縫","M",5.6]
[null,"  嵌縫及塞水路，連工帶料","M",5.6]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.53","W4a 180*100 鋁窗 (附摺疊紗窗)","樘",1]
[null,"  氟碳烤漆鋁窗","樘",1]
[null,"  推射子窗含五金","樘",2]
[null,"  摺疊紗窗","樘",2]
[null,"  8mm微反強化玻璃","才",20]
[null,"  無污染Silicone 防水填縫","M",5.6]
[null,"  嵌縫及塞水路，連工帶料","M",5.6]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.54","W5 180*100 鋁窗+防颱型百葉 (附摺疊紗窗)","樘",1]
[null,"  氟碳烤漆鋁窗","樘",1]
[null,"  推射子窗含五金","樘",1]
[null,"  摺疊紗窗","樘",1]
[null,"  8mm微反強化玻璃","才",10]
[null,"  安裝工資","樘",1]
[null,"  鋁質百葉窗，防颱型，氟碳烤漆(含不銹鋼防蟲網，三折式，透風率＞50.0%)","M2",0.9,null,null,"(風速22M/S,雨量200mm/hr,風吸入量3.0m3/s,阻雨率100%)"]
[null,"  防颱型鋁百葉組裝清潔(含固定五金)","M2",0.9]
[null,"  無污染Silicone 防水填縫","M",5.6]
[null,"  嵌縫及塞水路，連工帶料","M",5.6]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.55","W6 100*100 鋁窗 (附摺疊紗窗)","樘",1]
[null,"  氟碳烤漆鋁窗","樘",1]
[null,"  推射子窗含五金","樘",1]
[null,"  摺疊紗窗","樘",1]
[null,"  8mm微反強化玻璃","才",11]
[null,"  無污染Silicone 防水填縫","M",4]
[null,"  嵌縫及塞水路，連工帶料","M",4]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.56","W6a 100*100 鋁窗 (附摺疊紗窗)","樘",1]
[null,"  氟碳烤漆鋁窗","樘",1]
[null,"  推射子窗含五金","樘",1]
[null,"  摺疊紗窗","樘",1]
[null,"  8mm微反強化玻璃","才",11]
[null,"  無污染Silicone 防水填縫","M",4]
[null,"  嵌縫及塞水路，連工帶料","M",4]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.57","W7 100*50 鋁窗 (附摺疊紗窗)","樘",1]
[null,"  氟碳烤漆鋁窗","樘",1]
[null,"  推射子窗含五金","樘",1]
[null,"  摺疊紗窗","樘",1]
[null,"  8mm微反強化玻璃","才",6]
[null,"  無污染Silicone 防水填縫","M",3]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",3]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.58","W8 840*245 鋁窗+鋁門 (附紗窗,紗門)","樘",1]
[null,"  氟碳烤漆鋁窗","樘",1]
[null,"  橫拉窗及五金","樘",2]
[null,"  鋁門鉸鏈","片",4]
[null,"  不銹鋼圓管把手","組",1]
[null,"  門鎖","付",1]
[null,"  紗門及紗窗","樘",1]
[null,"  10mm微反強化玻璃","才",35]
[null,"  8mm微反強化玻璃","才",134]
[null,"  無污染Silicone 防水填縫","M",20.7]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",20.7]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.59","W9 100*100 鋁窗 (附紗窗)","樘",1]
[null,"  氟碳烤漆鋁窗","樘",1]
[null,"  橫拉窗及五金","樘",1]
[null,"  紗窗","樘",1]
[null,"  8mm微反強化玻璃","才",11]
[null,"  無污染Silicone 防水填縫","M",4]
[null,"  嵌縫及塞水路，水泥砂漿 1：2，連工帶料","M",4]
[null,"  安裝工資","樘",1]
[null,"  拆紙及清潔","樘",1]
[null,"  零星工料","式",1]
[null,"  計"]
["七.60","CW1 1214*4845 玻璃帷幕牆 含飾板","樘",1]
[null,"  帷幕現場吊線放樣","M2",588.20000000000005]
[null,"  一次鐵件製作與鋼構焊接","M2",588.20000000000005]
[null,"  帷幕框補鋼構架","M2",588.20000000000005]
[null,"  鋁框玻璃帷幕(含鋼梁處1.6mm烤漆鍍鋅彎板)","M2",588.20000000000005]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",6470]
[null,"  帷幕窗鋁飾板 60cm*15cm 含內骨架及補強","M",109.3]
[null,"  外框無污染矽膠防水填縫(含轉角)","M2",588.20000000000005]
[null,"  帷幕安裝工資","M2",588.20000000000005]
[null,"  拆紙及清潔","M2",588.20000000000005]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.61","CW2 3980.5*1185 玻璃帷幕牆","樘",1]
[null,"  帷幕現場吊線放樣","M2",451.9]
[null,"  一次鐵件製作與鋼構焊接","M2",451.9]
[null,"  帷幕框立料隱框補鋼構架","M2",451.9]
[null,"  鋁框玻璃帷幕(含鋼梁處1.6mm烤漆鍍鋅彎板)","M2",451.9]
[null,"  鋁框玻璃門樘","樘",2]
[null,"  隱藏式推開窗120*100","樘",3]
[null,"  摺疊紗窗","樘",3]
[null,"  雨遮四週內框防水板+防水填縫","M",25]
[null,"  二樓板防火帶及防水墩間鋁背板+防火矽酸鈣板夾岩棉","M",39.799999999999997]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",4845.8]
[null,"  超長玻璃製作安裝補助費","才",4845.8]
[null,"  地鉸鏈","付",2]
[null,"  90CM 不銹鋼圓管把手(內外)","付",2]
[null,"  輔助鎖","付",2]
[null,"  外框無污染矽膠防水填縫","M2",451.9]
[null,"  帷幕安裝工資","M2",451.9]
[null,"  拆紙及清潔","M2",451.9]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.62","CW3 219.5*490 玻璃帷幕牆","樘",1]
[null,"  一次鐵件製作與鋼構焊接","M2",10.8]
[null,"  帷幕框立料隱框補鋼構架","M2",10.8]
[null,"  鋁框玻璃帷幕","M2",10.8]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",118.3]
[null,"  超長玻璃製作安裝補助費","才",96.6]
[null,"  外框無污染矽膠防水填縫","M2",10.8]
[null,"  帷幕安裝工資","M2",10.8]
[null,"  拆紙及清潔","M2",10.8]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.63","CW4 219.5*490 玻璃帷幕牆 ","樘",1]
[null,"  一次鐵件製作與鋼構焊接","M2",10.8]
[null,"  帷幕框立料隱框補鋼構架","M2",10.8]
[null,"  鋁框玻璃帷幕","M2",10.8]
[null,"  隱藏式推開窗129.5*100","樘",1]
[null,"  摺疊紗窗","樘",1]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",118.3]
[null,"  外框無污染矽膠防水填縫","M2",10.8]
[null,"  帷幕安裝工資","M2",10.8]
[null,"  拆紙及清潔","M2",10.8]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.64","CW5 1498*400 玻璃帷幕牆 風除室","樘",1]
[null," 風除室位置放樣","M2",12.6]
[null," 風除室自立鋁框結構補強鋼構架","M2",12.6]
[null,"  頂板上下鋁包板(含燈具空調消防等設備配合開孔)","M2",12.6]
[null,"  鋁框玻璃帷幕","M2",59.9]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",659.1]
[null,"  雙開門自動門機","組",2]
[null,"  光電式安全裝置","組",2]
[null,"  輔助鎖","付",2]
[null,"  外框無污染矽膠防水填縫","M2",59.9]
[null,"  帷幕安裝工資","M2",59.9]
[null,"  拆紙及清潔","M2",59.9]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.65","CW6 979*335 玻璃帷幕牆","樘",1]
[null,"  帷幕框立料隱框補鋼構架","M2",32.799999999999997]
[null,"  鋁框玻璃帷幕","M2",32.799999999999997]
[null,"  隱藏式推開窗129.5*100","樘",2]
[null,"  摺疊紗窗","樘",2]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",360.8]
[null,"  外框無污染矽膠防水填縫","M2",32.799999999999997]
[null,"  帷幕安裝工資","M2",32.799999999999997]
[null,"  拆紙及清潔","M2",32.799999999999997]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.66","CW7 994*345 玻璃帷幕牆","樘",1]
[null,"  帷幕框立料隱框補鋼構架","M2",34.299999999999997]
[null,"  鋁框玻璃帷幕","M2",34.299999999999997]
[null,"  鋁框玻璃門樘","樘",2]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",377.2]
[null,"  地鉸鏈","付",2]
[null,"  60CM 不銹鋼圓管把手(內外)","付",2]
[null,"  輔助鎖","付",2]
[null,"  外框無污染矽膠防水填縫","M2",34.299999999999997]
[null,"  帷幕安裝工資","M2",34.299999999999997]
[null,"  拆紙及清潔","M2",34.299999999999997]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.67","CW8 898*345 玻璃帷幕牆","樘",1]
[null,"  帷幕框立料隱框補鋼構架","M2",31]
[null,"  鋁框玻璃帷幕","M2",31]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",340.8]
[null,"  外框無污染矽膠防水填縫","M2",31]
[null,"  帷幕安裝工資","M2",31]
[null,"  拆紙及清潔","M2",31]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.68","CW9 979*200 玻璃帷幕牆","樘",1]
[null,"  帷幕框立料隱框補鋼構架","M2",19.600000000000001]
[null,"  鋁框玻璃帷幕","M2",19.600000000000001]
[null,"  隱藏式推開窗129.5*100","樘",4]
[null,"  摺疊紗窗","樘",4]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",215.4]
[null,"  外框無污染矽膠防水填縫","M2",19.600000000000001]
[null,"  帷幕安裝工資","M2",19.600000000000001]
[null,"  拆紙及清潔","M2",19.600000000000001]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.69","CW10 968*305 玻璃帷幕牆","樘",1]
[null,"  帷幕框立料隱框補鋼構架","M2",29.5]
[null,"  鋁框玻璃帷幕","M2",29.5]
[null,"  鋁框玻璃門樘","樘",2]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",324.8]
[null,"  旗型鉸鏈 4.5\"*4.6mm 4培林","片",8]
[null,"  60CM 不銹鋼圓管把手(內外)","付",2]
[null,"  輔助鎖","付",2]
[null,"  外框無污染矽膠防水填縫","M2",29.5]
[null,"  帷幕安裝工資","M2",29.5]
[null,"  拆紙及清潔","M2",29.5]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.70","CW11 980*305 玻璃帷幕牆","樘",1]
[null,"  帷幕框立料隱框補鋼構架","M2",29.9]
[null,"  鋁框玻璃帷幕","M2",29.9]
[null,"  鋁框玻璃門樘","樘",1]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",328.8]
[null,"  旗型鉸鏈 4.5\"*4.6mm 4培林","片",4]
[null,"  60CM 不銹鋼圓管把手(內外)","付",1]
[null,"  輔助鎖","付",1]
[null,"  外框無污染矽膠防水填縫","M2",29.9]
[null,"  帷幕安裝工資","M2",29.9]
[null,"  拆紙及清潔","M2",29.9]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.71","CW12 1691*360 玻璃帷幕牆","樘",1]
[null,"  帷幕框立料隱框補鋼構架","M2",60.9]
[null,"  鋁框玻璃帷幕","M2",60.9]
[null,"  鋁框玻璃門樘","樘",1]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",634]
[null,"  旗型鉸鏈 4.5\"*4.6mm 4培林","片",4]
[null,"  60CM 不銹鋼圓管把手(內外)","付",1]
[null,"  輔助鎖","付",1]
[null,"  外框無污染矽膠防水填縫","M2",60.9]
[null,"  帷幕安裝工資","M2",60.9]
[null,"  拆紙及清潔","M2",60.9]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.72","CW13 180*5010 玻璃帷幕牆","樘",1]
[null,"  帷幕現場吊線放樣","M2",90.2]
[null,"  一次鐵件製作與鋼構焊接","M2",90.2]
[null,"  帷幕框補鋼構架","M2",90.2]
[null,"  鋁框玻璃帷幕(含鋼梁處1.6mm烤漆鍍鋅彎板)","M2",90.2]
[null,"  隱藏式推開窗 90*100","樘",9]
[null,"  摺疊紗窗","樘",9]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",992]
[null,"  外框無污染矽膠防水填縫(含轉角)","M2",90.2]
[null,"  帷幕安裝工資","M2",90.2]
[null,"  拆紙及清潔","M2",90.2]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.73","CW14 242*4110 玻璃帷幕牆","樘",1]
[null,"  帷幕現場吊線放樣","M2",99.5]
[null,"  一次鐵件製作與鋼構焊接","M2",99.5]
[null,"  帷幕框補鋼構架","M2",99.5]
[null,"  鋁框玻璃帷幕(含鋼梁處1.6mm烤漆鍍鋅彎板)","M2",99.5]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",1094.0999999999999]
[null,"  外框無污染矽膠防水填縫(含轉角)","M2",99.5]
[null,"  帷幕安裝工資","M2",99.5]
[null,"  拆紙及清潔","M2",99.5]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["七.74","CW15 3424*434*6 玻璃帷幕牆 含鋁飾板","樘",1]
[null,"  帷幕現場吊線放樣","M2",891.6]
[null,"  一次鐵件製作與鋼構焊接","M2",891.6]
[null,"  帷幕框補鋼構架","M2",891.6]
[null,"  鋁框玻璃帷幕(含鋼梁處1.6mm烤漆鍍鋅彎板)","M2",891.6]
[null,"  帷幕窗直立鋁飾板 80cm*15cm* H434cm 含內骨架及補強","片",59]
[null,"  二樓板防火帶及防水墩間鋁背板+防火矽酸鈣板夾岩棉","M",205.4]
[null,"  隱藏式推開窗 111~120*100","樘",18]
[null,"  摺疊紗窗","樘",18]
[null,"  8+8mm微反射雙熱硬化玻璃(含安裝)","才",9807.7000000000007]
[null,"  帷幕間樓板邊鋁包板 (含內骨料及填縫)","M",171.20000000000002]
[null,"  外框無污染矽膠防水填縫(含轉角)","M2",891.6]
[null,"  帷幕安裝工資","M2",891.6]
[null,"  拆紙及清潔","M2",891.6]
[null,"  零星工料及工具損耗","式",1]
[null,"  計"]
["八.1","無障礙安全梯A無障礙樓梯扶手TYPE A(H=90cm)","M",1]
[null,"  6mm不銹鋼板立柱及延伸固定板件等","kg",4.7]
[null,"  2\"φ不銹鋼管","M",1.1000000000000001]
[null,"  1 1/2\"φ不銹鋼管","M",1.1499999999999999]
[null,"  1 \"φ不銹鋼管","M",0.11]
[null,"  3/4\"φ不銹鋼管","M",3.3]
[null,"  氬焊製作及搬運","M",1]
[null,"  現場安裝及拋光處理","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.2","無障礙安全梯A無障礙樓梯扶手TYPE B(H=110cm)","M",1]
[null,"  6mm不銹鋼板立柱及延伸固定板件等","kg",5.64]
[null,"  2\"φ不銹鋼管","M",1.1000000000000001]
[null,"  1 1/2\"φ不銹鋼管","M",1.1499999999999999]
[null,"  1 \"φ不銹鋼管","M",0.11]
[null,"  3/4\"φ不銹鋼管","M",3.3]
[null,"  氬焊製作及搬運","M",1]
[null,"  現場安裝及拋光處理","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.3","無障礙安全梯A無障礙壁掛式扶手 安裝H=75cm","M",1]
[null,"  不銹鋼板固定件含延伸板件等","kg",0.8]
[null,"  1 1/2\"φ不銹鋼管","M",1.1499999999999999]
[null,"  氬焊製作及搬運","M",1]
[null,"  現場安裝及拋光處理","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.4","安全梯B樓梯扶手TYPE A(H=90cm)","M",1]
[null,"  6mm不銹鋼板立柱及延伸固定板件等","kg",4.2]
[null,"  2\"φ不銹鋼管","M",1.1000000000000001]
[null,"  1 \"φ不銹鋼管","M",0.11]
[null,"  3/4\"φ不銹鋼管","M",3.3]
[null,"  氬焊製作及搬運","M",1]
[null,"  現場安裝及拋光處理","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.5","安全梯B樓梯扶手TYPE B(H=110cm)","M",1]
[null,"  6mm不銹鋼板立柱及延伸固定板件等","kg",5.04]
[null,"  2\"φ不銹鋼管","M",1.1000000000000001]
[null,"  1 \"φ不銹鋼管","M",0.11]
[null,"  3/4\"φ不銹鋼管","M",3.3]
[null,"  氬焊製作及搬運","M",1]
[null,"  現場安裝及拋光處理","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.6","安全梯C樓梯扶手TYPE A(H=90cm)","M",1]
[null,"  6mm不銹鋼板立柱及延伸固定板件等","kg",4.2]
[null,"  2\"φ不銹鋼管","M",1.1000000000000001]
[null,"  1 \"φ不銹鋼管","M",0.11]
[null,"  3/4\"φ不銹鋼管","M",3.3]
[null,"  氬焊製作及搬運","M",1]
[null,"  現場安裝及拋光處理","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.7","安全梯C樓梯扶手TYPE B(H=110cm)","M",1]
[null,"  6mm不銹鋼板立柱及延伸固定板件等","kg",5.04]
[null,"  2\"φ不銹鋼管","M",1.1000000000000001]
[null,"  1 \"φ不銹鋼管","M",0.11]
[null,"  3/4\"φ不銹鋼管","M",3.3]
[null,"  氬焊製作及搬運","M",1]
[null,"  現場安裝及拋光處理","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.8","B2,B1層階梯無障礙樓梯扶手TYPE A(H=90cm)","M",1]
[null,"  6mm不銹鋼板立柱及延伸固定板件等","kg",4.7]
[null,"  2\"φ不銹鋼管","M",1.1000000000000001]
[null,"  1 1/2\"φ不銹鋼管","M",1.1499999999999999]
[null,"  1 \"φ不銹鋼管","M",0.11]
[null,"  3/4\"φ不銹鋼管","M",3.3]
[null,"  氬焊製作及搬運","M",1]
[null,"  現場安裝及拋光處理","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.9","B2,B1階梯無障礙壁掛式扶手 安裝H=75cm","M",1]
[null,"  不銹鋼板固定件含延伸板件等","kg",0.8]
[null,"  1 1/2\"φ不銹鋼管","M",1.1499999999999999]
[null,"  氬焊製作及搬運","M",1]
[null,"  現場安裝及拋光處理","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.10","上電梯機房階梯樓梯扶手TYPE A(H=90cm)","M",1]
[null,"  6mm不銹鋼板立柱及延伸固定板件等","kg",4.2]
[null,"  2\"φ不銹鋼管","M",1.1000000000000001]
[null,"  1 \"φ不銹鋼管","M",0.11]
[null,"  3/4\"φ不銹鋼管","M",3.3]
[null,"  氬焊製作及搬運","M",1]
[null,"  現場安裝及拋光處理","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.11","吊裝平台不銹鋼活動欄杆","M",1]
[null,"  6mm不銹鋼板延伸固定板件等","kg",2]
[null,"  2\"φ不銹鋼管","M",2.6]
[null,"  1 \"φ不銹鋼管","M",1.1000000000000001]
[null,"  立柱不銹鋼套管","式",1]
[null,"  氬焊製作及搬運","M",1]
[null,"  現場安裝及拋光處理","M",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.13","筏基水池氣密鑄鐵人孔蓋 80∮","組",1]
[null,"  鑄鐵氣密人孔蓋 80∮","組",1]
[null,"  人孔蓋安裝及四週水泥修補","組",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.19","廁所熱固性板隔間 含門扇,五金,掛鈎","間",1]
[null,"  熱固性樹脂板 19mm","M2",1.6]
[null,"  熱固性樹脂板 13mm","M2",3.2]
[null,"  不銹鋼固定件","組",1]
[null,"  回歸鉸鏈","組",1]
[null,"  不銹鋼指示門鎖","組",1]
[null,"  不銹鋼掛衣鉤","組",1]
[null,"  CNC車床栽切製作","間",1]
[null,"  現場組裝及清潔","間",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.20","小便斗隔板","片",1]
[null,"  熱固性樹脂板 13mm","M2",0.41]
[null,"  不銹鋼固定件","組",1]
[null,"  CNC車床栽切製作","片",1]
[null,"  現場組裝及清潔","片",1]
[null,"  零星工料","式",1]
[null,"  計"]
["八.28","茶水間組合式系統櫃含水槽及吊櫃 L=225CM","座",1]
[null,"  12mm人造石台面(含續接材料)","CM",225]
[null,"  廠製櫃體 L=225CM","座",1]
[null,"  單槽式不銹鋼水槽","個",1]
[null,"  吊櫃  L=225CM","座",1]
[null,"  運費反安裝技術工","座",1]
[null,"  小五金及另料","式",1]
[null,"  零星工料","式",1]
[null,"  計"]
["十1.1","景觀放樣","M2",1]
[null,"  測量儀器費"," 式",1]
[null,"  工資"," 工",1E-3]
[null,"  水平板及木料工具"," 式",1]
[null,"  損耗及其他"," 式",1]
[null," 計"]
["十1.2","整地","M2"]
[null,"  推土機，D6H，Cat","時",5.0000000000000001E-3]
[null,"  履帶式挖土機，鏟土容量0.70～0.79m3(含作業手、油料)","時",1E-3]
[null,"  大工"," 工",5.0000000000000001E-3]
[null,"  小工"," 工",5.0000000000000001E-3]
[null,"  零星工料"," 式",1]
[null,"  計"]
["十1.4","喬木苦楝現地移植入空氣盆，後定植 (H>300cm,W=250cm,∮>5cm)","株"]
[null,"  蒸散抑制劑","式",0.1]
[null,"  麻布及棉繩(吊搬襯墊)","株",0.1]
[null,"  吊車租用","天",0.05]
[null,"  挖土機","天",0.05]
[null,"  土球包覆(麻繩或其他包覆材包裹)","株",1]
[null,"  樹枝修剪工資","式",0.1]
[null,"  高密度泡棉","式",1]
[null,"  棉繩","式",1]
[null,"  圍籬鋼板圍籬","式",1]
[null,"  技術工(含樹木固定、種植、蒸散抑制劑噴灑)","工",0.6]
[null,"  小工","工",0.5]
[null,"  計"]
["十1.5","現況雜草石塊垃圾移除運棄","M2"]
[null,"  機具不分類，使用費","時",24]
[null,"  小工","工",15]
[null,"  廢方運棄，營建廢棄物處理（含運費及證明）","式",1]
[null,"  工具損耗及其他","式",1]
[null,"  計"]
["十2.11","喬木種植費","株",1]
[null,"  運費","株",1]
[null,"  種植費大工","工",0.6]
[null,"  種植費小工","工",0.6]
[null,"  新植灌水","式",1]
[null,"  杉木支架H180㎝*3支、H45cm*1支(ψ=6㎝) ","式",1]
[null,"  有機肥","KG",2]
[null,"  撫育費1年","式",1]
[null,"  工具損耗及其他","式",1]
[null,"  計"]
["十2.39","灌木種植費","株",1]
[null,"  種植工","工",0.01]
[null,"  施肥工","工",0.01]
[null,"  養護工","工",6.0000000000000001E-3]
[null,"  有機基追肥","KG",0.5]
[null,"  養護用具材料","式",1]
[null,"  苗木小搬運","式",1]
[null,"  搬運費","式",1]
[null,"  計"]
["十2.40","地被-類地毯草(密鋪)","M2"]
[null,"  假儉草毯","M2",1]
[null,"  植栽客土（含有機肥,5㎏/m3）","M3",0.1]
[null,"  技工（栽植、小搬運）","工",1.4999999999999999E-2]
[null,"  雜工（追肥、澆水、養護）","工",0.03]
[null,"  零星工料","式",1]
[null,"  計"]
["十2.44","地被-種植費","株"]
[null,"  種植工","工",1E-3]
["  ","  施肥工","工",1E-3]
[null,"  養護工","工",1E-3]
[null,"  有機基追肥","KG",0.5]
[null,"  養護用具材料","式",1]
[null,"  苗木小搬運","式",1]
[null,"  搬運費","式",1]
[null,"  計"]
["十2.45","植栽，客土，砂質壤土 ","M3"]
[null,"  石塊、棄土運棄","式",1]
[null,"  人工整地","工",0.01]
[null,"  砂質壤土","M3",1]
[null,"  人工小搬運","工",0.05]
[null,"  計"]
["十3.1","燒面花崗岩-60*60CM(黑灰)","M2"]
[null,"  花崗岩-60*60CM*3CM(黑灰)","㎡",1]
[null,"  燒面加工","㎡",1]
[null,"  4000psi 混凝土15cm工料","㎡",1]
[null,"  3#點焊鋼筋網","㎡",1]
[null,"  舖設工資","㎡",1]
[null,"  零星工料(含切磋及損耗)","式",1]
[null,"  計"]
["十3.2","噴砂面高壓混凝土磚-30*30CM*8CM(白)","M2"]
[null,"  高壓混凝土磚(透心)","㎡",1]
[null,"  磚面噴砂加工","㎡",1]
[null,"  基礎夯實工","工",0.01]
[null,"  碎石級配","m3",0.15]
[null,"  2分石","m3",0.04]
[null,"  舖設工資","㎡",1]
[null,"  零星工料(含切磋及損耗)","式",1]
[null,"  計"]
["十3.3","噴砂面高壓混凝土磚-30*30CM*8CM(灰)錯落排列","M2"]
[null,"  高壓混凝土磚(透心)","㎡",1]
[null,"  磚面噴砂加工","㎡",1]
[null,"  基礎夯實工","工",0.01]
[null,"  碎石級配","m3",0.15]
[null,"  2分石","m3",0.04]
[null,"  舖設工資","㎡",1]
[null,"  零星工料(含切磋及損耗)","式",1]
[null,"  計"]
["十3.4","噴砂面高壓混凝土磚-30*30CM*8CM(灰)線性排列","M2"]
[null,"  高壓混凝土磚(透心)","㎡",1]
[null,"  磚面噴砂加工","㎡",1]
[null,"  基礎夯實工","工",0.01]
[null,"  碎石級配","m3",0.15]
[null,"  2分石","m3",0.04]
[null,"  舖設工資","㎡",1]
[null,"  零星工料(含切磋及損耗)","式",1]
[null,"  計"]
["十3.5","噴砂面高壓混凝土磚-30*30CM*8CM(黑灰)線性排列","M2"]
[null,"  高壓混凝土磚(透心)","㎡",1]
[null,"  磚面噴砂加工","㎡",1]
[null,"  基礎夯實工","工",0.01]
[null,"  碎石級配","m3",0.15]
[null,"  2分石","m3",0.04]
[null,"  舖設工資","㎡",1]
[null,"  零星工料(含切磋及損耗)","式",1]
[null,"  計"]
["十3.6","噴砂面高壓混凝土磚-10*10CM*8CM(黑灰)","M2"]
[null,"  高壓混凝土磚(透心)","㎡",1]
[null,"  磚面噴砂加工","㎡",1]
[null,"  基礎夯實工","工",0.01]
[null,"  碎石級配","m3",0.15]
[null,"  2分石","m3",0.04]
[null,"  舖設工資","㎡",1]
[null,"  零星工料(含切磋及損耗)","式",1]
[null,"  計"]
["十3.7","燒面花崗岩緣石-寬15CM(黑灰)T=8CM","M"]
[null,"  花崗石","m",1]
[null,"  燒面加工","m",1]
[null,"  水泥砂漿","m3",0.03]
[null,"  舖設工資","m",1]
[null,"  基礎夯實","工",0.01]
[null,"  零星工料(含切磋及損耗)","式",1]
[null,"  計"]
["十3.8","玄武岩踏片步道","M2"]
[null,"  玄武岩踏片","㎡",1]
[null,"  人工小搬運","工",0.1]
[null,"  襯墊砂","m3",0.04]
[null,"  舖設工資","㎡",1]
[null,"  零星工料(含切磋及損耗)","式",1]
[null,"  計"]
["十3.9","入口處人行道鋪面復原(高壓混凝土磚40x20cm，TH=8cm丁掛排列，表面處理及顏色同現有人行道)","M2"]
[null,"  高壓混凝土磚(透心)","㎡",1]
[null,"  磚面加工","㎡",1]
[null,"  基礎夯實","工",0.01]
[null,"  碎石級配","m3",0.15]
[null,"  2分石","m3",0.04]
[null,"  舖設工資","㎡",1]
[null,"  零星工料(含切磋及損耗)","式",1]
[null,"  計"]